<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="1.27" unitdist="mm" unit="mm" style="lines" multiple="1" display="yes" altdistance="0.127" altunitdist="mm" altunit="mm"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="2" name="Route2" color="1" fill="3" visible="no" active="yes"/>
<layer number="3" name="Route3" color="4" fill="3" visible="no" active="yes"/>
<layer number="4" name="Route4" color="1" fill="4" visible="no" active="yes"/>
<layer number="5" name="Route5" color="4" fill="4" visible="no" active="yes"/>
<layer number="6" name="Route6" color="1" fill="8" visible="no" active="yes"/>
<layer number="7" name="Route7" color="4" fill="8" visible="no" active="yes"/>
<layer number="8" name="Route8" color="1" fill="2" visible="no" active="yes"/>
<layer number="9" name="Route9" color="4" fill="2" visible="no" active="yes"/>
<layer number="10" name="Route10" color="1" fill="7" visible="no" active="yes"/>
<layer number="11" name="Route11" color="4" fill="7" visible="no" active="yes"/>
<layer number="12" name="Route12" color="1" fill="5" visible="no" active="yes"/>
<layer number="13" name="Route13" color="4" fill="5" visible="no" active="yes"/>
<layer number="14" name="Route14" color="1" fill="6" visible="no" active="yes"/>
<layer number="15" name="Route15" color="4" fill="6" visible="no" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="yes" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
</layers>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electrolytic Capacitors,Ceramic Capacitors &amp; Film Capacitors&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle &lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiCap does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

Eagle Version 6, Library Revision 2015a, 08.04.2015&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="2.6X1.6X1(BXCXA)">
<smd name="2" x="-1.8" y="0" dx="2.6" dy="1.6" layer="1"/>
<smd name="1" x="1.8" y="0" dx="2.6" dy="1.6" layer="1"/>
<wire x1="-2.15" y1="2.15" x2="1.35" y2="2.15" width="0.127" layer="21"/>
<wire x1="-2.15" y1="-2.15" x2="-2.15" y2="-0.8" width="0.127" layer="21"/>
<wire x1="-2.15" y1="-2.15" x2="1.35" y2="-2.15" width="0.127" layer="21"/>
<wire x1="-2.15" y1="2.15" x2="-2.15" y2="0.8" width="0.127" layer="21"/>
<wire x1="1.35" y1="2.15" x2="2.15" y2="1.35" width="0.127" layer="21"/>
<wire x1="1.35" y1="-2.15" x2="2.15" y2="-1.35" width="0.127" layer="21"/>
<wire x1="-3.35" y1="2.4" x2="3.35" y2="2.4" width="0.127" layer="39"/>
<wire x1="-3.35" y1="-2.4" x2="3.35" y2="-2.4" width="0.127" layer="39"/>
<wire x1="-3.35" y1="2.4" x2="-3.35" y2="-2.4" width="0.127" layer="39"/>
<wire x1="3.35" y1="2.4" x2="3.35" y2="-2.4" width="0.127" layer="39"/>
<text x="-4.4" y="4.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-5.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="2.15" y1="1.35" x2="2.15" y2="0.8" width="0.127" layer="21"/>
<wire x1="2.15" y1="-1.35" x2="2.15" y2="-0.8" width="0.127" layer="21"/>
</package>
<package name="3X1.6X1.4(BXCXA)">
<smd name="2" x="-2.2" y="0" dx="3" dy="1.6" layer="1"/>
<smd name="1" x="2.2" y="0" dx="3" dy="1.6" layer="1"/>
<wire x1="-2.65" y1="2.65" x2="1.65" y2="2.65" width="0.127" layer="21"/>
<wire x1="-2.65" y1="-2.65" x2="-2.65" y2="-0.8" width="0.127" layer="21"/>
<wire x1="-2.65" y1="-2.65" x2="1.65" y2="-2.65" width="0.127" layer="21"/>
<wire x1="-2.65" y1="2.65" x2="-2.65" y2="0.8" width="0.127" layer="21"/>
<wire x1="1.65" y1="2.65" x2="2.65" y2="1.65" width="0.127" layer="21"/>
<wire x1="1.65" y1="-2.65" x2="2.65" y2="-1.65" width="0.127" layer="21"/>
<wire x1="-3.95" y1="2.9" x2="3.95" y2="2.9" width="0.127" layer="39"/>
<wire x1="-3.95" y1="-2.9" x2="3.95" y2="-2.9" width="0.127" layer="39"/>
<wire x1="-3.95" y1="2.9" x2="-3.95" y2="-2.9" width="0.127" layer="39"/>
<wire x1="3.95" y1="2.9" x2="3.95" y2="-2.9" width="0.127" layer="39"/>
<text x="-4.4" y="4.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-6.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="2.65" y1="1.65" x2="2.65" y2="0.8" width="0.127" layer="21"/>
<wire x1="2.65" y1="-1.65" x2="2.65" y2="-0.8" width="0.127" layer="21"/>
</package>
<package name="3.5X1.6X2.1(BXCXA)">
<smd name="2" x="-2.8" y="0" dx="3.5" dy="1.6" layer="1"/>
<smd name="1" x="2.8" y="0" dx="3.5" dy="1.6" layer="1"/>
<wire x1="-3.3" y1="3.3" x2="1.75" y2="3.3" width="0.127" layer="21"/>
<wire x1="-3.3" y1="-3.3" x2="-3.3" y2="-0.8" width="0.127" layer="21"/>
<wire x1="-3.3" y1="-3.3" x2="1.75" y2="-3.3" width="0.127" layer="21"/>
<wire x1="-3.3" y1="3.3" x2="-3.3" y2="0.8" width="0.127" layer="21"/>
<wire x1="1.75" y1="3.3" x2="3.3" y2="1.75" width="0.127" layer="21"/>
<wire x1="1.75" y1="-3.3" x2="3.3" y2="-1.75" width="0.127" layer="21"/>
<wire x1="-4.8" y1="3.55" x2="4.8" y2="3.55" width="0.127" layer="39"/>
<wire x1="-4.8" y1="-3.55" x2="4.8" y2="-3.55" width="0.127" layer="39"/>
<wire x1="-4.8" y1="3.55" x2="-4.8" y2="-3.55" width="0.127" layer="39"/>
<wire x1="4.8" y1="3.55" x2="4.8" y2="-3.55" width="0.127" layer="39"/>
<text x="-4.4" y="4.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-5.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="3.3" y1="1.75" x2="3.3" y2="0.8" width="0.127" layer="21"/>
<wire x1="3.3" y1="-1.75" x2="3.3" y2="-0.8" width="0.127" layer="21"/>
</package>
<package name="4.4X1.9X4.3(BXCXA)">
<smd name="2" x="-4.35" y="0" dx="4.4" dy="1.9" layer="1"/>
<smd name="1" x="4.35" y="0" dx="4.4" dy="1.9" layer="1"/>
<wire x1="-5.15" y1="5.15" x2="3.15" y2="5.15" width="0.127" layer="21"/>
<wire x1="-5.15" y1="-5.15" x2="-5.15" y2="-0.95" width="0.127" layer="21"/>
<wire x1="-5.15" y1="-5.15" x2="3.15" y2="-5.15" width="0.127" layer="21"/>
<wire x1="-5.15" y1="5.15" x2="-5.15" y2="0.95" width="0.127" layer="21"/>
<wire x1="3.15" y1="5.15" x2="5.15" y2="3.15" width="0.127" layer="21"/>
<wire x1="3.15" y1="-5.15" x2="5.15" y2="-3.15" width="0.127" layer="21"/>
<wire x1="-6.8" y1="5.4" x2="6.8" y2="5.4" width="0.127" layer="39"/>
<wire x1="-6.8" y1="-5.4" x2="6.8" y2="-5.4" width="0.127" layer="39"/>
<wire x1="-6.8" y1="5.4" x2="-6.8" y2="-5.4" width="0.127" layer="39"/>
<wire x1="6.8" y1="5.4" x2="6.8" y2="-5.4" width="0.127" layer="39"/>
<text x="-4.4" y="6.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-7.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="5.15" y1="3.15" x2="5.15" y2="0.95" width="0.127" layer="21"/>
<wire x1="5.15" y1="-3.15" x2="5.15" y2="-0.95" width="0.127" layer="21"/>
</package>
<package name="4.2X1.9X2.8(BXCXA)">
<smd name="2" x="-3.5" y="0" dx="4.2" dy="1.9" layer="1"/>
<smd name="1" x="3.5" y="0" dx="4.2" dy="1.9" layer="1"/>
<wire x1="-4.15" y1="4.15" x2="2.35" y2="4.15" width="0.127" layer="21"/>
<wire x1="-4.15" y1="-4.15" x2="-4.15" y2="-0.95" width="0.127" layer="21"/>
<wire x1="-4.15" y1="-4.15" x2="2.35" y2="-4.15" width="0.127" layer="21"/>
<wire x1="-4.15" y1="4.15" x2="-4.15" y2="0.95" width="0.127" layer="21"/>
<wire x1="2.35" y1="4.15" x2="4.15" y2="2.35" width="0.127" layer="21"/>
<wire x1="2.35" y1="-4.15" x2="4.15" y2="-2.35" width="0.127" layer="21"/>
<wire x1="-5.85" y1="4.4" x2="5.85" y2="4.4" width="0.127" layer="39"/>
<wire x1="-5.85" y1="-4.4" x2="5.85" y2="-4.4" width="0.127" layer="39"/>
<wire x1="-5.85" y1="4.4" x2="-5.85" y2="-4.4" width="0.127" layer="39"/>
<wire x1="5.85" y1="4.4" x2="5.85" y2="-4.4" width="0.127" layer="39"/>
<text x="-4.4" y="6.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-7.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="4.15" y1="2.35" x2="4.15" y2="0.95" width="0.127" layer="21"/>
<wire x1="4.15" y1="-2.35" x2="4.15" y2="-0.95" width="0.127" layer="21"/>
</package>
<package name="4.5X1.6X2.1(BXCXA)">
<smd name="2" x="-3.3" y="0" dx="4.5" dy="1.6" layer="1"/>
<smd name="1" x="3.3" y="0" dx="4.5" dy="1.6" layer="1"/>
<wire x1="-4.15" y1="4.15" x2="2.35" y2="4.15" width="0.127" layer="21"/>
<wire x1="-4.15" y1="-4.15" x2="-4.15" y2="-0.95" width="0.127" layer="21"/>
<wire x1="-4.15" y1="-4.15" x2="2.35" y2="-4.15" width="0.127" layer="21"/>
<wire x1="-4.15" y1="4.15" x2="-4.15" y2="0.95" width="0.127" layer="21"/>
<wire x1="2.35" y1="4.15" x2="4.15" y2="2.35" width="0.127" layer="21"/>
<wire x1="2.35" y1="-4.15" x2="4.15" y2="-2.35" width="0.127" layer="21"/>
<wire x1="-5.8" y1="4.4" x2="5.8" y2="4.4" width="0.127" layer="39"/>
<wire x1="-5.8" y1="-4.4" x2="5.8" y2="-4.4" width="0.127" layer="39"/>
<wire x1="-5.8" y1="4.4" x2="-5.8" y2="-4.4" width="0.127" layer="39"/>
<wire x1="5.8" y1="4.4" x2="5.8" y2="-4.4" width="0.127" layer="39"/>
<text x="-4.4" y="6.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-7.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="4.15" y1="2.35" x2="4.15" y2="0.95" width="0.127" layer="21"/>
<wire x1="4.15" y1="-2.35" x2="4.15" y2="-0.95" width="0.127" layer="21"/>
</package>
<package name="5.8X2.5X4.3(BXCXA)">
<smd name="2" x="-5.05" y="0" dx="5.8" dy="2.5" layer="1"/>
<smd name="1" x="5.05" y="0" dx="5.8" dy="2.5" layer="1"/>
<wire x1="-6.75" y1="6.75" x2="4.25" y2="6.75" width="0.127" layer="21"/>
<wire x1="-6.75" y1="-6.75" x2="-6.75" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-6.75" y1="-6.75" x2="4.25" y2="-6.75" width="0.127" layer="21"/>
<wire x1="-6.75" y1="6.75" x2="-6.75" y2="1.25" width="0.127" layer="21"/>
<wire x1="4.25" y1="6.75" x2="6.75" y2="4.25" width="0.127" layer="21"/>
<wire x1="4.25" y1="-6.75" x2="6.75" y2="-4.25" width="0.127" layer="21"/>
<wire x1="-8.2" y1="7" x2="8.2" y2="7" width="0.127" layer="39"/>
<wire x1="-8.2" y1="-7" x2="8.2" y2="-7" width="0.127" layer="39"/>
<wire x1="-8.2" y1="7" x2="-8.2" y2="-7" width="0.127" layer="39"/>
<wire x1="8.2" y1="7" x2="8.2" y2="-7" width="0.127" layer="39"/>
<text x="-4.4" y="8.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-9.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="6.75" y1="4.25" x2="6.75" y2="1.25" width="0.127" layer="21"/>
<wire x1="6.75" y1="-4.25" x2="6.75" y2="-1.25" width="0.127" layer="21"/>
</package>
<package name="6.5X3.5X6(BXCXA)">
<smd name="2" x="-6.25" y="0" dx="6.5" dy="3.5" layer="1"/>
<smd name="1" x="6.25" y="0" dx="6.5" dy="3.5" layer="1"/>
<wire x1="-8.55" y1="8.55" x2="6.05" y2="8.55" width="0.127" layer="21"/>
<wire x1="-8.55" y1="-8.55" x2="-8.55" y2="-1.75" width="0.127" layer="21"/>
<wire x1="-8.55" y1="-8.55" x2="6.05" y2="-8.55" width="0.127" layer="21"/>
<wire x1="-8.55" y1="8.55" x2="-8.55" y2="1.75" width="0.127" layer="21"/>
<wire x1="6.05" y1="8.55" x2="8.55" y2="6.05" width="0.127" layer="21"/>
<wire x1="6.05" y1="-8.55" x2="8.55" y2="-6.05" width="0.127" layer="21"/>
<wire x1="-9.75" y1="8.8" x2="9.7" y2="8.8" width="0.127" layer="39"/>
<wire x1="-9.75" y1="-8.8" x2="9.75" y2="-8.8" width="0.127" layer="39"/>
<wire x1="-9.75" y1="8.8" x2="-9.75" y2="-8.8" width="0.127" layer="39"/>
<wire x1="9.7" y1="8.8" x2="9.75" y2="-8.8" width="0.127" layer="39"/>
<text x="-4.4" y="10.4" size="1.27" layer="25">&gt;NAME</text>
<text x="-4.4" y="-11.6" size="1.27" layer="27">&gt;VALUE</text>
<wire x1="8.55" y1="6.05" x2="8.55" y2="1.75" width="0.127" layer="21"/>
<wire x1="8.55" y1="-6.05" x2="8.55" y2="-1.75" width="0.127" layer="21"/>
</package>
<package name="22X10X2(DXPXΦ)">
<pad name="1" x="5" y="0" drill="2" shape="square"/>
<pad name="2" x="-5" y="0" drill="2"/>
<circle x="0" y="0" radius="11" width="0.127" layer="21"/>
<circle x="0" y="0" radius="11.25" width="0.127" layer="39"/>
<text x="-2.54" y="13.43" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-14.7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="25X10X2(DXPXΦ)">
<pad name="1" x="5" y="0" drill="2" shape="square"/>
<pad name="2" x="-5" y="0" drill="2"/>
<circle x="0" y="0" radius="12.5" width="0.127" layer="21"/>
<circle x="0" y="0" radius="12.75" width="0.127" layer="39"/>
<text x="-2.54" y="15.43" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-16.7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="30X10X2(DXPXΦ)">
<pad name="1" x="5" y="0" drill="2" shape="square"/>
<pad name="2" x="-5" y="0" drill="2"/>
<circle x="0" y="0" radius="15" width="0.127" layer="21"/>
<circle x="0" y="0" radius="15.25" width="0.127" layer="39"/>
<text x="-2.54" y="17.43" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-18.7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="35X10X2(DXPXΦ)">
<pad name="1" x="5" y="0" drill="2" shape="square"/>
<pad name="2" x="-5" y="0" drill="2"/>
<circle x="0" y="0" radius="17.5" width="0.127" layer="21"/>
<circle x="0" y="0" radius="17.75" width="0.127" layer="39"/>
<text x="-2.54" y="19.43" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-20.7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="40X10X2(DXPXΦ)">
<pad name="1" x="5" y="0" drill="2" shape="square"/>
<pad name="2" x="-5" y="0" drill="2"/>
<circle x="0" y="0" radius="20" width="0.127" layer="21"/>
<circle x="0" y="0" radius="20.25" width="0.127" layer="39"/>
<text x="-2.54" y="22.43" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-23.7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="5X2X0.8(DXAXB)">
<pad name="1" x="1" y="0" drill="0.8" shape="square"/>
<pad name="2" x="-1" y="0" drill="0.8"/>
<circle x="0" y="0" radius="2.5" width="0.127" layer="21"/>
<circle x="0" y="0" radius="2.75" width="0.127" layer="39"/>
<text x="-2.54" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="6.3X2.5X0.8(DXAXB)">
<pad name="1" x="1.25" y="0" drill="0.8" shape="square"/>
<pad name="2" x="-1.25" y="0" drill="0.8"/>
<circle x="0" y="0" radius="3.15" width="0.127" layer="21"/>
<circle x="0" y="0" radius="3.4" width="0.127" layer="39"/>
<text x="-2.54" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="8X3.5X0.8(DXAXB)">
<pad name="1" x="1.75" y="0" drill="0.8" shape="square"/>
<pad name="2" x="-1.75" y="0" drill="0.8"/>
<circle x="0" y="0" radius="4" width="0.127" layer="21"/>
<circle x="0" y="0" radius="4.25" width="0.127" layer="39"/>
<text x="-2.54" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="10X5X0.9(DXAXB)">
<pad name="1" x="2.5" y="0" drill="0.9" shape="square"/>
<pad name="2" x="-2.5" y="0" drill="0.9"/>
<circle x="0" y="0" radius="5" width="0.127" layer="21"/>
<circle x="0" y="0" radius="5.25" width="0.127" layer="39"/>
<text x="-2.54" y="7.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-8.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="13X5X0.9(DXAXB)">
<pad name="1" x="2.5" y="0" drill="0.9" shape="square"/>
<pad name="2" x="-2.5" y="0" drill="0.9"/>
<circle x="0" y="0" radius="6.5" width="0.127" layer="21"/>
<circle x="0" y="0" radius="6.75" width="0.127" layer="39"/>
<text x="-2.54" y="7.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-8.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="16X7.5X1.1(DXAXB)">
<pad name="1" x="3.75" y="0" drill="1.1" shape="square"/>
<pad name="2" x="-3.75" y="0" drill="1.1"/>
<circle x="0" y="0" radius="8" width="0.127" layer="21"/>
<circle x="0" y="0" radius="8.25" width="0.127" layer="39"/>
<text x="-2.54" y="10.89" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-12.16" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="18X7.5X1.1(DXAXB)">
<pad name="1" x="3.75" y="0" drill="1.1" shape="square"/>
<pad name="2" x="-3.75" y="0" drill="1.1"/>
<circle x="0" y="0" radius="9" width="0.127" layer="21"/>
<circle x="0" y="0" radius="9.25" width="0.127" layer="39"/>
<text x="-2.54" y="10.89" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-12.16" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="22X10X1.1(DXAXB)">
<pad name="1" x="5" y="0" drill="1.1" shape="square"/>
<pad name="2" x="-5" y="0" drill="1.1"/>
<circle x="0" y="0" radius="11" width="0.127" layer="21"/>
<circle x="0" y="0" radius="11.25" width="0.127" layer="39"/>
<text x="-2.54" y="13.43" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-14.7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="8X3.5X0.9(DXAXB)">
<pad name="1" x="1.75" y="0" drill="0.9" shape="square"/>
<pad name="2" x="-1.75" y="0" drill="0.9"/>
<circle x="0" y="0" radius="4" width="0.127" layer="21"/>
<circle x="0" y="0" radius="4.25" width="0.127" layer="39"/>
<text x="-2.54" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="6.3X2.5X0.9(DXAXB)">
<pad name="1" x="1.25" y="0" drill="0.9" shape="square"/>
<pad name="2" x="-1.25" y="0" drill="0.9"/>
<circle x="0" y="0" radius="3.15" width="0.127" layer="21"/>
<circle x="0" y="0" radius="3.4" width="0.127" layer="39"/>
<text x="-2.54" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-CSGP_0402">
<description>&lt;b&gt;WCAP-CSGP_0402

&lt;br&gt;&lt;br&gt;&lt;/b&gt;size code LxW; 1 x 0.5 ;</description>
<smd name="1" x="-0.5" y="0" dx="0.5" dy="0.5" layer="1"/>
<smd name="2" x="0.5" y="0" dx="0.5" dy="0.5" layer="1"/>
<wire x1="-0.5" y1="0.25" x2="-0.5" y2="-0.25" width="0.127" layer="51"/>
<wire x1="0.5" y1="-0.25" x2="0.5" y2="0.25" width="0.127" layer="51"/>
<wire x1="-0.5" y1="0.25" x2="-0.25" y2="0.25" width="0.127" layer="51"/>
<wire x1="-0.5" y1="-0.25" x2="-0.25" y2="-0.25" width="0.127" layer="51"/>
<wire x1="0.25" y1="-0.25" x2="0.5" y2="-0.25" width="0.127" layer="51"/>
<wire x1="0.25" y1="0.25" x2="0.5" y2="0.25" width="0.127" layer="51"/>
<wire x1="-0.25" y1="0.25" x2="0.25" y2="0.25" width="0.127" layer="21"/>
<wire x1="-0.25" y1="-0.25" x2="0.25" y2="-0.25" width="0.127" layer="21"/>
<wire x1="-1" y1="0.5" x2="1" y2="0.5" width="0.127" layer="39"/>
<wire x1="1" y1="0.5" x2="1" y2="-0.5" width="0.127" layer="39"/>
<wire x1="1" y1="-0.5" x2="-1" y2="-0.5" width="0.127" layer="39"/>
<wire x1="-1" y1="-0.5" x2="-1" y2="0.5" width="0.127" layer="39"/>
<text x="-1.25" y="0.75" size="0.4064" layer="25">&gt;NAME</text>
<text x="-1.25" y="-1.25" size="0.4064" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-CSGP_0603_WAVE">
<description>&lt;b&gt;WCAP-CSGP_0603
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Solder type: Wave

&lt;br&gt;&lt;/b&gt;&lt;/b&gt;&lt;br&gt;size code LxW; 1.6 x 0.8 ;</description>
<smd name="1" x="-0.85" y="0" dx="0.7" dy="0.8" layer="1"/>
<smd name="2" x="0.85" y="0" dx="0.7" dy="0.8" layer="1"/>
<wire x1="-0.8" y1="0.4" x2="-0.8" y2="-0.4" width="0.127" layer="51"/>
<wire x1="0.8" y1="-0.4" x2="0.8" y2="0.4" width="0.127" layer="51"/>
<wire x1="-0.8" y1="0.4" x2="-0.5" y2="0.4" width="0.127" layer="51"/>
<wire x1="-0.8" y1="-0.4" x2="-0.5" y2="-0.4" width="0.127" layer="51"/>
<wire x1="0.5" y1="-0.4" x2="0.8" y2="-0.4" width="0.127" layer="51"/>
<wire x1="0.5" y1="0.4" x2="0.8" y2="0.4" width="0.127" layer="51"/>
<wire x1="-1.45" y1="0.65" x2="1.45" y2="0.65" width="0.127" layer="39"/>
<wire x1="1.45" y1="0.65" x2="1.45" y2="-0.65" width="0.127" layer="39"/>
<wire x1="-1.45" y1="-0.65" x2="-1.45" y2="0.65" width="0.127" layer="39"/>
<text x="-1.25" y="1" size="0.4064" layer="25">&gt;NAME</text>
<text x="-1.25" y="-1.4" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-0.5" y1="0.4" x2="0.5" y2="0.4" width="0.127" layer="21"/>
<wire x1="-0.5" y1="-0.4" x2="0.5" y2="-0.4" width="0.127" layer="21"/>
<wire x1="-1.45" y1="-0.65" x2="1.45" y2="-0.65" width="0.127" layer="39"/>
</package>
<package name="WCAP-CSGP_0603_REFLOW">
<description>&lt;b&gt;WCAP-CSGP_0603
&lt;br&gt;
&lt;br&gt;Solder type: Reflow
&lt;br&gt;&lt;br&gt;&lt;/b&gt;size code LxW; 1,6 x 0,8 ;</description>
<smd name="1" x="-0.75" y="0" dx="0.8" dy="0.8" layer="1"/>
<smd name="2" x="0.75" y="0" dx="0.8" dy="0.8" layer="1"/>
<wire x1="-0.8" y1="0.4" x2="-0.8" y2="-0.4" width="0.127" layer="51"/>
<wire x1="0.8" y1="-0.4" x2="0.8" y2="0.4" width="0.127" layer="51"/>
<wire x1="-0.8" y1="0.4" x2="-0.35" y2="0.4" width="0.127" layer="51"/>
<wire x1="-0.8" y1="-0.4" x2="-0.35" y2="-0.4" width="0.127" layer="51"/>
<wire x1="0.35" y1="-0.4" x2="0.8" y2="-0.4" width="0.127" layer="51"/>
<wire x1="0.35" y1="0.4" x2="0.8" y2="0.4" width="0.127" layer="51"/>
<wire x1="-1.4" y1="0.65" x2="1.4" y2="0.65" width="0.127" layer="39"/>
<wire x1="1.4" y1="0.65" x2="1.4" y2="-0.65" width="0.127" layer="39"/>
<wire x1="-1.4" y1="-0.65" x2="-1.4" y2="0.65" width="0.127" layer="39"/>
<text x="-1.25" y="1" size="0.4064" layer="25">&gt;NAME</text>
<text x="-1.25" y="-1.4" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-0.35" y1="0.4" x2="0.35" y2="0.4" width="0.127" layer="21"/>
<wire x1="-0.35" y1="-0.4" x2="0.35" y2="-0.4" width="0.127" layer="21"/>
<wire x1="-1.4" y1="-0.65" x2="1.4" y2="-0.65" width="0.127" layer="39"/>
</package>
<package name="WCAP-CSGP_0805_WAVE">
<description>&lt;b&gt;WCAP-CSGP_0805
&lt;br&gt;
&lt;br&gt;Solder type: Wave

&lt;br&gt;&lt;br&gt;&lt;/b&gt;size code LxW: 2 x 1.25 ;</description>
<smd name="1" x="-1.15" y="0" dx="0.9" dy="1.3" layer="1"/>
<smd name="2" x="1.15" y="0" dx="0.9" dy="1.3" layer="1"/>
<wire x1="-1" y1="0.625" x2="-1" y2="-0.625" width="0.127" layer="51"/>
<wire x1="1" y1="-0.625" x2="1" y2="0.625" width="0.127" layer="51"/>
<wire x1="-1" y1="0.625" x2="-0.7" y2="0.625" width="0.127" layer="51"/>
<wire x1="-1" y1="-0.625" x2="-0.7" y2="-0.625" width="0.127" layer="51"/>
<wire x1="0.7" y1="-0.625" x2="1" y2="-0.625" width="0.127" layer="51"/>
<wire x1="0.7" y1="0.625" x2="1" y2="0.625" width="0.127" layer="51"/>
<wire x1="-1.85" y1="0.9" x2="1.85" y2="0.9" width="0.127" layer="39"/>
<wire x1="1.85" y1="0.9" x2="1.85" y2="-0.9" width="0.127" layer="39"/>
<wire x1="-1.85" y1="-0.9" x2="-1.85" y2="0.9" width="0.127" layer="39"/>
<text x="-1.5" y="1.4" size="0.4064" layer="25">&gt;NAME</text>
<text x="-1.5" y="-1.8" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-0.7" y1="0.625" x2="0.7" y2="0.625" width="0.127" layer="21"/>
<wire x1="-1.85" y1="-0.9" x2="1.85" y2="-0.9" width="0.127" layer="39"/>
<wire x1="-0.7" y1="-0.625" x2="0.7" y2="-0.625" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSGP_0805_REFLOW">
<description>&lt;b&gt;WCAP-CSGP_0805
&lt;br&gt;&lt;br&gt;Solder type: Reflow

&lt;br&gt;&lt;br&gt;&lt;/b&gt;size code LxW; 2 x 1.25 ;</description>
<smd name="1" x="-0.95" y="0" dx="0.9" dy="1.3" layer="1"/>
<smd name="2" x="0.95" y="0" dx="0.9" dy="1.3" layer="1"/>
<wire x1="-1" y1="0.625" x2="-1" y2="-0.625" width="0.127" layer="51"/>
<wire x1="1" y1="-0.625" x2="1" y2="0.625" width="0.127" layer="51"/>
<wire x1="-1" y1="0.625" x2="-0.5" y2="0.625" width="0.127" layer="51"/>
<wire x1="-1" y1="-0.625" x2="-0.5" y2="-0.625" width="0.127" layer="51"/>
<wire x1="0.5" y1="-0.625" x2="1" y2="-0.625" width="0.127" layer="51"/>
<wire x1="0.5" y1="0.625" x2="1" y2="0.625" width="0.127" layer="51"/>
<wire x1="-1.65" y1="0.9" x2="1.65" y2="0.9" width="0.127" layer="39"/>
<wire x1="1.65" y1="0.9" x2="1.65" y2="-0.9" width="0.127" layer="39"/>
<wire x1="-1.65" y1="-0.9" x2="-1.65" y2="0.9" width="0.127" layer="39"/>
<text x="-1.5" y="1.4" size="0.4064" layer="25">&gt;NAME</text>
<text x="-1.5" y="-1.8" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-0.5" y1="0.625" x2="0.5" y2="0.625" width="0.127" layer="21"/>
<wire x1="-1.65" y1="-0.9" x2="1.65" y2="-0.9" width="0.127" layer="39"/>
<wire x1="-0.5" y1="-0.625" x2="0.5" y2="-0.625" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSGP_1206">
<description>&lt;b&gt;&lt;br&gt;WCAP-CSGP_1206
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; size code LxW; 3.2 x 1.6 ;</description>
<smd name="1" x="-1.55" y="0" dx="0.9" dy="1.6" layer="1"/>
<smd name="2" x="1.55" y="0" dx="0.9" dy="1.6" layer="1"/>
<wire x1="-1.6" y1="0.8" x2="-1.6" y2="-0.8" width="0.127" layer="51"/>
<wire x1="1.6" y1="-0.8" x2="1.6" y2="0.8" width="0.127" layer="51"/>
<wire x1="-1.6" y1="0.8" x2="-1.1" y2="0.8" width="0.127" layer="51"/>
<wire x1="-1.6" y1="-0.8" x2="-1.1" y2="-0.8" width="0.127" layer="51"/>
<wire x1="1.1" y1="-0.8" x2="1.6" y2="-0.8" width="0.127" layer="51"/>
<wire x1="1.1" y1="0.8" x2="1.6" y2="0.8" width="0.127" layer="51"/>
<wire x1="-2.25" y1="1.05" x2="2.25" y2="1.05" width="0.127" layer="39"/>
<wire x1="2.25" y1="1.05" x2="2.25" y2="-1.05" width="0.127" layer="39"/>
<wire x1="-2.25" y1="-1.05" x2="-2.25" y2="1.05" width="0.127" layer="39"/>
<text x="-1.5" y="1.4" size="0.4064" layer="25">&gt;NAME</text>
<text x="-1.5" y="-1.8" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-1.1" y1="0.8" x2="1.1" y2="0.8" width="0.127" layer="21"/>
<wire x1="-2.25" y1="-1.05" x2="2.25" y2="-1.05" width="0.127" layer="39"/>
<wire x1="-1.1" y1="-0.8" x2="1.1" y2="-0.8" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSGP_1210">
<description>&lt;b&gt;WCAP-CSGP_1210
&lt;br&gt;
&lt;/b&gt;&lt;br&gt; size code LxW; 3.2 x 2.5 ;</description>
<smd name="1" x="-1.55" y="0" dx="0.9" dy="2.5" layer="1"/>
<smd name="2" x="1.55" y="0" dx="0.9" dy="2.5" layer="1"/>
<wire x1="-1.6" y1="1.25" x2="-1.6" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.6" y1="-1.25" x2="1.6" y2="1.25" width="0.127" layer="51"/>
<wire x1="-1.6" y1="1.25" x2="-1.1" y2="1.25" width="0.127" layer="51"/>
<wire x1="-1.6" y1="-1.25" x2="-1.1" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.1" y1="-1.25" x2="1.6" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.1" y1="1.25" x2="1.6" y2="1.25" width="0.127" layer="51"/>
<wire x1="-2.25" y1="1.5" x2="2.25" y2="1.5" width="0.127" layer="39"/>
<wire x1="2.25" y1="1.5" x2="2.25" y2="-1.5" width="0.127" layer="39"/>
<wire x1="-2.25" y1="-1.5" x2="-2.25" y2="1.5" width="0.127" layer="39"/>
<text x="-2" y="1.8" size="0.4064" layer="25">&gt;NAME</text>
<text x="-2" y="-2.2" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-1.1" y1="1.25" x2="1.1" y2="1.25" width="0.127" layer="21"/>
<wire x1="-2.25" y1="-1.5" x2="2.25" y2="-1.5" width="0.127" layer="39"/>
<wire x1="-1.1" y1="-1.25" x2="1.1" y2="-1.25" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSGP_1812">
<description>&lt;b&gt;WCAP-CSGP_1812
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;size code LxW; 4.5 x 3.2 ;</description>
<smd name="1" x="-2.2" y="0" dx="0.9" dy="3.8" layer="1"/>
<smd name="2" x="2.2" y="0" dx="0.9" dy="3.8" layer="1"/>
<wire x1="-2.25" y1="1.9" x2="-2.25" y2="-1.9" width="0.127" layer="51"/>
<wire x1="2.25" y1="-1.9" x2="2.25" y2="1.9" width="0.127" layer="51"/>
<wire x1="-2.25" y1="1.9" x2="-1.75" y2="1.9" width="0.127" layer="51"/>
<wire x1="-2.25" y1="-1.9" x2="-1.75" y2="-1.9" width="0.127" layer="51"/>
<wire x1="1.75" y1="-1.9" x2="2.25" y2="-1.9" width="0.127" layer="51"/>
<wire x1="1.75" y1="1.9" x2="2.25" y2="1.9" width="0.127" layer="51"/>
<wire x1="-2.9" y1="2.15" x2="2.9" y2="2.15" width="0.127" layer="39"/>
<wire x1="2.9" y1="2.15" x2="2.9" y2="-2.15" width="0.127" layer="39"/>
<wire x1="-2.9" y1="-2.15" x2="-2.9" y2="2.15" width="0.127" layer="39"/>
<text x="-2.65" y="2.5" size="0.4064" layer="25">&gt;NAME</text>
<text x="-2.65" y="-2.9" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-1.75" y1="1.9" x2="1.75" y2="1.9" width="0.127" layer="21"/>
<wire x1="-2.9" y1="-2.15" x2="2.9" y2="-2.15" width="0.127" layer="39"/>
<wire x1="-1.75" y1="-1.9" x2="1.75" y2="-1.9" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSSA_1808">
<description>&lt;b&gt;WCAP-CSSA_1808
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;size code LxW; 4.5 x 2 ;</description>
<smd name="1" x="-2.175" y="0" dx="1.05" dy="2.3" layer="1"/>
<smd name="2" x="2.175" y="0" dx="1.05" dy="2.3" layer="1"/>
<wire x1="-2.25" y1="1" x2="-2.25" y2="-1" width="0.127" layer="51"/>
<wire x1="2.25" y1="-1" x2="2.25" y2="1" width="0.127" layer="51"/>
<wire x1="-2.25" y1="1" x2="-1.65" y2="1" width="0.127" layer="51"/>
<wire x1="-2.25" y1="-1" x2="-1.65" y2="-1" width="0.127" layer="51"/>
<wire x1="1.65" y1="-1" x2="2.25" y2="-1" width="0.127" layer="51"/>
<wire x1="1.65" y1="1" x2="2.25" y2="1" width="0.127" layer="51"/>
<wire x1="-2.925" y1="1.4" x2="2.925" y2="1.4" width="0.127" layer="39"/>
<wire x1="2.925" y1="1.4" x2="2.925" y2="-1.4" width="0.127" layer="39"/>
<wire x1="-2.925" y1="-1.4" x2="-2.925" y2="1.4" width="0.127" layer="39"/>
<text x="-2.65" y="2.5" size="0.4064" layer="25">&gt;NAME</text>
<text x="-2.65" y="-2.9" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-1.65" y1="1" x2="1.65" y2="1" width="0.127" layer="21"/>
<wire x1="-2.925" y1="-1.4" x2="2.925" y2="-1.4" width="0.127" layer="39"/>
<wire x1="-1.65" y1="-1" x2="1.65" y2="-1" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSSA_1812">
<description>&lt;b&gt;WCAP-CSSA_1812
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;size code LxW ; 4.5 x 3.2 ;</description>
<smd name="1" x="-2.2" y="0" dx="0.9" dy="3.8" layer="1"/>
<smd name="2" x="2.2" y="0" dx="0.9" dy="3.8" layer="1"/>
<wire x1="-2.25" y1="1.6" x2="-2.25" y2="-1.6" width="0.127" layer="51"/>
<wire x1="2.25" y1="-1.6" x2="2.25" y2="1.6" width="0.127" layer="51"/>
<wire x1="-2.25" y1="1.6" x2="-1.75" y2="1.6" width="0.127" layer="51"/>
<wire x1="-2.25" y1="-1.6" x2="-1.75" y2="-1.6" width="0.127" layer="51"/>
<wire x1="1.75" y1="-1.6" x2="2.25" y2="-1.6" width="0.127" layer="51"/>
<wire x1="1.75" y1="1.6" x2="2.25" y2="1.6" width="0.127" layer="51"/>
<wire x1="-2.9" y1="2.15" x2="2.9" y2="2.15" width="0.127" layer="39"/>
<wire x1="2.9" y1="2.15" x2="2.9" y2="-2.15" width="0.127" layer="39"/>
<wire x1="-2.9" y1="-2.15" x2="-2.9" y2="2.15" width="0.127" layer="39"/>
<text x="-2.65" y="2.5" size="0.4064" layer="25">&gt;NAME</text>
<text x="-2.65" y="-2.9" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-1.75" y1="1.6" x2="1.75" y2="1.6" width="0.127" layer="21"/>
<wire x1="-2.9" y1="-2.15" x2="2.9" y2="-2.15" width="0.127" layer="39"/>
<wire x1="-1.75" y1="-1.6" x2="1.75" y2="-1.6" width="0.127" layer="21"/>
</package>
<package name="WCAP-CSSA_2211">
<description>&lt;b&gt;WCAP-CSSA_2211
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;size code LxW ; 5.7 x 2.8 ;</description>
<smd name="1" x="-2.825" y="0" dx="1.35" dy="3.7" layer="1"/>
<smd name="2" x="2.825" y="0" dx="1.35" dy="3.7" layer="1"/>
<wire x1="-2.85" y1="1.4" x2="-2.85" y2="-1.4" width="0.127" layer="51"/>
<wire x1="2.85" y1="-1.4" x2="2.85" y2="1.4" width="0.127" layer="51"/>
<wire x1="-2.85" y1="1.4" x2="-2.15" y2="1.4" width="0.127" layer="51"/>
<wire x1="-2.85" y1="-1.4" x2="-2.15" y2="-1.4" width="0.127" layer="51"/>
<wire x1="2.15" y1="-1.4" x2="2.85" y2="-1.4" width="0.127" layer="51"/>
<wire x1="2.15" y1="1.4" x2="2.85" y2="1.4" width="0.127" layer="51"/>
<wire x1="-3.75" y1="2.1" x2="3.75" y2="2.1" width="0.127" layer="39"/>
<wire x1="3.75" y1="2.1" x2="3.75" y2="-2.1" width="0.127" layer="39"/>
<wire x1="-3.75" y1="-2.1" x2="-3.75" y2="2.1" width="0.127" layer="39"/>
<text x="-2.65" y="2.5" size="0.4064" layer="25">&gt;NAME</text>
<text x="-2.65" y="-2.9" size="0.4064" layer="27">&gt;VALUE</text>
<wire x1="-2.15" y1="1.4" x2="2.15" y2="1.4" width="0.127" layer="21"/>
<wire x1="-3.75" y1="-2.1" x2="3.75" y2="-2.1" width="0.127" layer="39"/>
<wire x1="-2.15" y1="-1.4" x2="2.15" y2="-1.4" width="0.127" layer="21"/>
</package>
<package name="WCAP-FTX2_7.5X11X10X6">
<pad name="1" x="-3.75" y="0" drill="0.9"/>
<pad name="2" x="3.75" y="0" drill="0.9"/>
<wire x1="-5.5" y1="3" x2="5.5" y2="3" width="0.127" layer="21"/>
<wire x1="5.5" y1="3" x2="5.5" y2="-3" width="0.127" layer="21"/>
<wire x1="5.5" y1="-3" x2="-5.5" y2="-3" width="0.127" layer="21"/>
<wire x1="-5.5" y1="-3" x2="-5.5" y2="3" width="0.127" layer="21"/>
<wire x1="-5.75" y1="3.25" x2="5.75" y2="3.25" width="0.127" layer="39"/>
<wire x1="5.75" y1="3.25" x2="5.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="5.75" y1="-3.25" x2="-5.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-5.75" y1="-3.25" x2="-5.75" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_7.5X10X12X6">
<pad name="1" x="-3.75" y="0" drill="0.9"/>
<pad name="2" x="3.75" y="0" drill="0.9"/>
<wire x1="-5" y1="3" x2="5" y2="3" width="0.127" layer="21"/>
<wire x1="5" y1="3" x2="5" y2="-3" width="0.127" layer="21"/>
<wire x1="5" y1="-3" x2="-5" y2="-3" width="0.127" layer="21"/>
<wire x1="-5" y1="-3" x2="-5" y2="3" width="0.127" layer="21"/>
<wire x1="-5.25" y1="3.25" x2="5.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="5.25" y1="3.25" x2="5.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="5.25" y1="-3.25" x2="-5.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-5.25" y1="-3.25" x2="-5.25" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_10X13X10X5">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="2.5" x2="6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="2.5" x2="6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-2.5" x2="-6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-2.5" x2="-6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="2.75" x2="6.75" y2="2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="2.75" x2="6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-2.75" x2="-6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-2.75" x2="-6.75" y2="2.75" width="0.127" layer="39"/>
<text x="-6.35" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.35" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_10X13X11X5">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="2.5" x2="6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="2.5" x2="6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-2.5" x2="-6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-2.5" x2="-6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="2.75" x2="6.75" y2="2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="2.75" x2="6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-2.75" x2="-6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-2.75" x2="-6.75" y2="2.75" width="0.127" layer="39"/>
<text x="-6.35" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.35" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_10X13X9.5X4.5">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="2.25" x2="6.5" y2="2.25" width="0.127" layer="21"/>
<wire x1="6.5" y1="2.25" x2="6.5" y2="-2.25" width="0.127" layer="21"/>
<wire x1="6.5" y1="-2.25" x2="-6.5" y2="-2.25" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-2.25" x2="-6.5" y2="2.25" width="0.127" layer="21"/>
<wire x1="-6.75" y1="2.5" x2="6.75" y2="2.5" width="0.127" layer="39"/>
<wire x1="6.75" y1="2.5" x2="6.75" y2="-2.5" width="0.127" layer="39"/>
<wire x1="6.75" y1="-2.5" x2="-6.75" y2="-2.5" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-2.5" x2="-6.75" y2="2.5" width="0.127" layer="39"/>
<text x="-6.35" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.35" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_10X13X13X7">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="3.5" x2="6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="3.5" x2="6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-3.5" x2="-6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-3.5" x2="-6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="3.75" x2="6.75" y2="3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="3.75" x2="6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-3.75" x2="-6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-3.75" x2="-6.75" y2="3.75" width="0.127" layer="39"/>
<text x="-6.08" y="4.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.08" y="-6.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_10X13X12X7">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="3.5" x2="6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="3.5" x2="6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-3.5" x2="-6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-3.5" x2="-6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="3.75" x2="6.75" y2="3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="3.75" x2="6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-3.75" x2="-6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-3.75" x2="-6.75" y2="3.75" width="0.127" layer="39"/>
<text x="-6.08" y="4.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.08" y="-6.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_10X13X14X8">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="4" x2="6.5" y2="4" width="0.127" layer="21"/>
<wire x1="6.5" y1="4" x2="6.5" y2="-4" width="0.127" layer="21"/>
<wire x1="6.5" y1="-4" x2="-6.5" y2="-4" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-4" x2="-6.5" y2="4" width="0.127" layer="21"/>
<wire x1="-6.75" y1="4.25" x2="6.75" y2="4.25" width="0.127" layer="39"/>
<wire x1="6.75" y1="4.25" x2="6.75" y2="-4.25" width="0.127" layer="39"/>
<wire x1="6.75" y1="-4.25" x2="-6.75" y2="-4.25" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-4.25" x2="-6.75" y2="4.25" width="0.127" layer="39"/>
<text x="-6.08" y="4.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.08" y="-6.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_12.5X15X11.5X6">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="3" x2="7.5" y2="3" width="0.127" layer="21"/>
<wire x1="7.5" y1="3" x2="7.5" y2="-3" width="0.127" layer="21"/>
<wire x1="7.5" y1="-3" x2="-7.5" y2="-3" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-3" x2="-7.5" y2="3" width="0.127" layer="21"/>
<wire x1="-7.75" y1="3.25" x2="7.75" y2="3.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="3.25" x2="7.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="-3.25" x2="-7.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-3.25" x2="-7.75" y2="3.25" width="0.127" layer="39"/>
<text x="-7.35" y="4.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-7.35" y="-6.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_12.5X15X12.5X7">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="3.5" x2="7.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="7.5" y1="3.5" x2="7.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="7.5" y1="-3.5" x2="-7.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-3.5" x2="-7.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="-7.75" y1="3.75" x2="7.75" y2="3.75" width="0.127" layer="39"/>
<wire x1="7.75" y1="3.75" x2="7.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="7.75" y1="-3.75" x2="-7.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-3.75" x2="-7.75" y2="3.75" width="0.127" layer="39"/>
<text x="-7.35" y="4.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-7.35" y="-6.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_12.5X15X14X8.5">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="4.25" x2="7.5" y2="4.25" width="0.127" layer="21"/>
<wire x1="7.5" y1="4.25" x2="7.5" y2="-4.25" width="0.127" layer="21"/>
<wire x1="7.5" y1="-4.25" x2="-7.5" y2="-4.25" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-4.25" x2="-7.5" y2="4.25" width="0.127" layer="21"/>
<wire x1="-7.75" y1="4.5" x2="7.75" y2="4.5" width="0.127" layer="39"/>
<wire x1="7.75" y1="4.5" x2="7.75" y2="-4.5" width="0.127" layer="39"/>
<wire x1="7.75" y1="-4.5" x2="-7.75" y2="-4.5" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-4.5" x2="-7.75" y2="4.5" width="0.127" layer="39"/>
<text x="-7.35" y="4.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-7.35" y="-6.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_12.5X15X16X10">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="5" x2="7.5" y2="5" width="0.127" layer="21"/>
<wire x1="7.5" y1="5" x2="7.5" y2="-5" width="0.127" layer="21"/>
<wire x1="7.5" y1="-5" x2="-7.5" y2="-5" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-5" x2="-7.5" y2="5" width="0.127" layer="21"/>
<wire x1="-7.75" y1="5.25" x2="7.75" y2="5.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="5.25" x2="7.75" y2="-5.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="-5.25" x2="-7.75" y2="-5.25" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-5.25" x2="-7.75" y2="5.25" width="0.127" layer="39"/>
<text x="-7.35" y="5.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-7.35" y="-7.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X11X5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="2.5" x2="9" y2="2.5" width="0.127" layer="21"/>
<wire x1="9" y1="2.5" x2="9" y2="-2.5" width="0.127" layer="21"/>
<wire x1="9" y1="-2.5" x2="-9" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-9" y1="-2.5" x2="-9" y2="2.5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="2.75" x2="9.25" y2="2.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="2.75" x2="9.25" y2="-2.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="-2.75" x2="-9.25" y2="-2.75" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-2.75" x2="-9.25" y2="2.75" width="0.127" layer="39"/>
<text x="-8.62" y="3.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-4.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X12X6">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3" x2="9" y2="3" width="0.127" layer="21"/>
<wire x1="9" y1="3" x2="9" y2="-3" width="0.127" layer="21"/>
<wire x1="9" y1="-3" x2="-9" y2="-3" width="0.127" layer="21"/>
<wire x1="-9" y1="-3" x2="-9" y2="3" width="0.127" layer="21"/>
<wire x1="-9.25" y1="3.25" x2="9.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="3.25" x2="9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-3.25" x2="-9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-3.25" x2="-9.25" y2="3.25" width="0.127" layer="39"/>
<text x="-8.62" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X13.5X7.5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3.75" x2="9" y2="3.75" width="0.127" layer="21"/>
<wire x1="9" y1="3.75" x2="9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="9" y1="-3.75" x2="-9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-9" y1="-3.75" x2="-9" y2="3.75" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4" x2="9.25" y2="4" width="0.127" layer="39"/>
<wire x1="9.25" y1="4" x2="9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4" x2="-9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4" x2="-9.25" y2="4" width="0.127" layer="39"/>
<text x="-8.62" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X11.5X6">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3" x2="9" y2="3" width="0.127" layer="21"/>
<wire x1="9" y1="3" x2="9" y2="-3" width="0.127" layer="21"/>
<wire x1="9" y1="-3" x2="-9" y2="-3" width="0.127" layer="21"/>
<wire x1="-9" y1="-3" x2="-9" y2="3" width="0.127" layer="21"/>
<wire x1="-9.25" y1="3.25" x2="9.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="3.25" x2="9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-3.25" x2="-9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-3.25" x2="-9.25" y2="3.25" width="0.127" layer="39"/>
<text x="-8.62" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X14.5X7.5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3.75" x2="9" y2="3.75" width="0.127" layer="21"/>
<wire x1="9" y1="3.75" x2="9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="9" y1="-3.75" x2="-9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-9" y1="-3.75" x2="-9" y2="3.75" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4" x2="9.25" y2="4" width="0.127" layer="39"/>
<wire x1="9.25" y1="4" x2="9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4" x2="-9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4" x2="-9.25" y2="4" width="0.127" layer="39"/>
<text x="-8.62" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X14.5X8.5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="4.25" x2="9" y2="4.25" width="0.127" layer="21"/>
<wire x1="9" y1="4.25" x2="9" y2="-4.25" width="0.127" layer="21"/>
<wire x1="9" y1="-4.25" x2="-9" y2="-4.25" width="0.127" layer="21"/>
<wire x1="-9" y1="-4.25" x2="-9" y2="4.25" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4.5" x2="9.25" y2="4.5" width="0.127" layer="39"/>
<wire x1="9.25" y1="4.5" x2="9.25" y2="-4.5" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4.5" x2="-9.25" y2="-4.5" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4.5" x2="-9.25" y2="4.5" width="0.127" layer="39"/>
<text x="-8.62" y="5.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-7.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X14X8">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="4" x2="9" y2="4" width="0.127" layer="21"/>
<wire x1="9" y1="4" x2="9" y2="-4" width="0.127" layer="21"/>
<wire x1="9" y1="-4" x2="-9" y2="-4" width="0.127" layer="21"/>
<wire x1="-9" y1="-4" x2="-9" y2="4" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4.25" x2="9.25" y2="4.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="4.25" x2="9.25" y2="-4.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4.25" x2="-9.25" y2="-4.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4.25" x2="-9.25" y2="4.25" width="0.127" layer="39"/>
<text x="-8.62" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X15X9">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="4.5" x2="9" y2="4.5" width="0.127" layer="21"/>
<wire x1="9" y1="4.5" x2="9" y2="-4.5" width="0.127" layer="21"/>
<wire x1="9" y1="-4.5" x2="-9" y2="-4.5" width="0.127" layer="21"/>
<wire x1="-9" y1="-4.5" x2="-9" y2="4.5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4.75" x2="9.25" y2="4.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="4.75" x2="9.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4.75" x2="-9.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4.75" x2="-9.25" y2="4.75" width="0.127" layer="39"/>
<text x="-8.62" y="5.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-7.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_15X18X16X10">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="5" x2="9" y2="5" width="0.127" layer="21"/>
<wire x1="9" y1="5" x2="9" y2="-5" width="0.127" layer="21"/>
<wire x1="9" y1="-5" x2="-9" y2="-5" width="0.127" layer="21"/>
<wire x1="-9" y1="-5" x2="-9" y2="5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="5.25" x2="9.25" y2="5.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="5.25" x2="9.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-5.25" x2="-9.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-5.25" x2="-9.25" y2="5.25" width="0.127" layer="39"/>
<text x="-8.62" y="5.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-8.62" y="-7.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X15X6">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="3" x2="13" y2="3" width="0.127" layer="21"/>
<wire x1="13" y1="3" x2="13" y2="-3" width="0.127" layer="21"/>
<wire x1="13" y1="-3" x2="-13" y2="-3" width="0.127" layer="21"/>
<wire x1="-13" y1="-3" x2="-13" y2="3" width="0.127" layer="21"/>
<wire x1="-13.25" y1="3.25" x2="13.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="3.25" x2="13.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="-3.25" x2="-13.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-3.25" x2="-13.25" y2="3.25" width="0.127" layer="39"/>
<text x="-12.43" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X16.5X7.5">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="3.75" x2="13" y2="3.75" width="0.127" layer="21"/>
<wire x1="13" y1="3.75" x2="13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="13" y1="-3.75" x2="-13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-13" y1="-3.75" x2="-13" y2="3.75" width="0.127" layer="21"/>
<wire x1="-13.25" y1="4" x2="13.25" y2="4" width="0.127" layer="39"/>
<wire x1="13.25" y1="4" x2="13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="13.25" y1="-4" x2="-13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-4" x2="-13.25" y2="4" width="0.127" layer="39"/>
<text x="-12.43" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X15X7.5">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="3.75" x2="13" y2="3.75" width="0.127" layer="21"/>
<wire x1="13" y1="3.75" x2="13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="13" y1="-3.75" x2="-13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-13" y1="-3.75" x2="-13" y2="3.75" width="0.127" layer="21"/>
<wire x1="-13.25" y1="4" x2="13.25" y2="4" width="0.127" layer="39"/>
<wire x1="13.25" y1="4" x2="13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="13.25" y1="-4" x2="-13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-4" x2="-13.25" y2="4" width="0.127" layer="39"/>
<text x="-12.43" y="4.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-5.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X18X9">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="4.5" x2="13" y2="4.5" width="0.127" layer="21"/>
<wire x1="13" y1="4.5" x2="13" y2="-4.5" width="0.127" layer="21"/>
<wire x1="13" y1="-4.5" x2="-13" y2="-4.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-4.5" x2="-13" y2="4.5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="4.75" x2="13.25" y2="4.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="4.75" x2="13.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="-4.75" x2="-13.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-4.75" x2="-13.25" y2="4.75" width="0.127" layer="39"/>
<text x="-12.43" y="5.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-7.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X20X11">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="5.5" x2="13" y2="5.5" width="0.127" layer="21"/>
<wire x1="13" y1="5.5" x2="13" y2="-5.5" width="0.127" layer="21"/>
<wire x1="13" y1="-5.5" x2="-13" y2="-5.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-5.5" x2="-13" y2="5.5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="5.75" x2="13.25" y2="5.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="5.75" x2="13.25" y2="-5.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="-5.75" x2="-13.25" y2="-5.75" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-5.75" x2="-13.25" y2="5.75" width="0.127" layer="39"/>
<text x="-12.43" y="7.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-8.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X21X10">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="5" x2="13" y2="5" width="0.127" layer="21"/>
<wire x1="13" y1="5" x2="13" y2="-5" width="0.127" layer="21"/>
<wire x1="13" y1="-5" x2="-13" y2="-5" width="0.127" layer="21"/>
<wire x1="-13" y1="-5" x2="-13" y2="5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="5.25" x2="13.25" y2="5.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="5.25" x2="13.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="-5.25" x2="-13.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-5.25" x2="-13.25" y2="5.25" width="0.127" layer="39"/>
<text x="-12.43" y="5.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-7.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_22.5X26X25X15">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="7.5" x2="13" y2="7.5" width="0.127" layer="21"/>
<wire x1="13" y1="7.5" x2="13" y2="-7.5" width="0.127" layer="21"/>
<wire x1="13" y1="-7.5" x2="-13" y2="-7.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-7.5" x2="-13" y2="7.5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="7.75" x2="13.25" y2="7.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="7.75" x2="13.25" y2="-7.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="-7.75" x2="-13.25" y2="-7.75" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-7.75" x2="-13.25" y2="7.75" width="0.127" layer="39"/>
<text x="-12.43" y="8.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-12.43" y="-10.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_27.5X31X20X10.5">
<pad name="1" x="-13.75" y="0" drill="1.1"/>
<pad name="2" x="13.75" y="0" drill="1.1"/>
<wire x1="-15.5" y1="5.25" x2="15.5" y2="5.25" width="0.127" layer="21"/>
<wire x1="15.5" y1="5.25" x2="15.5" y2="-5.25" width="0.127" layer="21"/>
<wire x1="15.5" y1="-5.25" x2="-15.5" y2="-5.25" width="0.127" layer="21"/>
<wire x1="-15.5" y1="-5.25" x2="-15.5" y2="5.25" width="0.127" layer="21"/>
<wire x1="-15.75" y1="5.5" x2="15.75" y2="5.5" width="0.127" layer="39"/>
<wire x1="15.75" y1="5.5" x2="15.75" y2="-5.5" width="0.127" layer="39"/>
<wire x1="15.75" y1="-5.5" x2="-15.75" y2="-5.5" width="0.127" layer="39"/>
<wire x1="-15.75" y1="-5.5" x2="-15.75" y2="5.5" width="0.127" layer="39"/>
<text x="-14.97" y="6.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-14.97" y="-7.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_27.5X31X22X13">
<pad name="1" x="-13.75" y="0" drill="1.1"/>
<pad name="2" x="13.75" y="0" drill="1.1"/>
<wire x1="-15.5" y1="6.5" x2="15.5" y2="6.5" width="0.127" layer="21"/>
<wire x1="15.5" y1="6.5" x2="15.5" y2="-6.5" width="0.127" layer="21"/>
<wire x1="15.5" y1="-6.5" x2="-15.5" y2="-6.5" width="0.127" layer="21"/>
<wire x1="-15.5" y1="-6.5" x2="-15.5" y2="6.5" width="0.127" layer="21"/>
<wire x1="-15.75" y1="6.75" x2="15.75" y2="6.75" width="0.127" layer="39"/>
<wire x1="15.75" y1="6.75" x2="15.75" y2="-6.75" width="0.127" layer="39"/>
<wire x1="15.75" y1="-6.75" x2="-15.75" y2="-6.75" width="0.127" layer="39"/>
<wire x1="-15.75" y1="-6.75" x2="-15.75" y2="6.75" width="0.127" layer="39"/>
<text x="-14.97" y="7.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-14.97" y="-8.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_27.5X31X29X15.5">
<pad name="1" x="-13.75" y="0" drill="1.1"/>
<pad name="2" x="13.75" y="0" drill="1.1"/>
<wire x1="-15.5" y1="7.75" x2="15.5" y2="7.75" width="0.127" layer="21"/>
<wire x1="15.5" y1="7.75" x2="15.5" y2="-7.75" width="0.127" layer="21"/>
<wire x1="15.5" y1="-7.75" x2="-15.5" y2="-7.75" width="0.127" layer="21"/>
<wire x1="-15.5" y1="-7.75" x2="-15.5" y2="7.75" width="0.127" layer="21"/>
<wire x1="-15.75" y1="8" x2="15.75" y2="8" width="0.127" layer="39"/>
<wire x1="15.75" y1="8" x2="15.75" y2="-8" width="0.127" layer="39"/>
<wire x1="15.75" y1="-8" x2="-15.75" y2="-8" width="0.127" layer="39"/>
<wire x1="-15.75" y1="-8" x2="-15.75" y2="8" width="0.127" layer="39"/>
<text x="-14.97" y="8.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-14.97" y="-10.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTX2_37.5X41.5X35.5X22.5">
<pad name="1" x="-18.75" y="0" drill="1.3"/>
<pad name="2" x="18.75" y="0" drill="1.3"/>
<wire x1="-20.75" y1="11.25" x2="20.75" y2="11.25" width="0.127" layer="21"/>
<wire x1="20.75" y1="11.25" x2="20.75" y2="-11.25" width="0.127" layer="21"/>
<wire x1="20.75" y1="-11.25" x2="-20.75" y2="-11.25" width="0.127" layer="21"/>
<wire x1="-20.75" y1="-11.25" x2="-20.75" y2="11.25" width="0.127" layer="21"/>
<wire x1="-21" y1="11.5" x2="21" y2="11.5" width="0.127" layer="39"/>
<wire x1="21" y1="11.5" x2="21" y2="-11.5" width="0.127" layer="39"/>
<wire x1="21" y1="-11.5" x2="-21" y2="-11.5" width="0.127" layer="39"/>
<wire x1="-21" y1="-11.5" x2="-21" y2="11.5" width="0.127" layer="39"/>
<text x="-20.05" y="12.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-20.05" y="-14.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_7.5X11X10X6">
<pad name="1" x="-3.75" y="0" drill="0.9"/>
<pad name="2" x="3.75" y="0" drill="0.9"/>
<wire x1="-5.5" y1="3" x2="5.5" y2="3" width="0.127" layer="21"/>
<wire x1="5.5" y1="3" x2="5.5" y2="-3" width="0.127" layer="21"/>
<wire x1="5.5" y1="-3" x2="-5.5" y2="-3" width="0.127" layer="21"/>
<wire x1="-5.5" y1="-3" x2="-5.5" y2="3" width="0.127" layer="21"/>
<wire x1="-5.75" y1="3.25" x2="5.75" y2="3.25" width="0.127" layer="39"/>
<wire x1="5.75" y1="3.25" x2="5.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="5.75" y1="-3.25" x2="-5.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-5.75" y1="-3.25" x2="-5.75" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_7.5X10X12X6">
<pad name="1" x="-3.75" y="0" drill="0.9"/>
<pad name="2" x="3.75" y="0" drill="0.9"/>
<wire x1="-5" y1="3" x2="5" y2="3" width="0.127" layer="21"/>
<wire x1="5" y1="3" x2="5" y2="-3" width="0.127" layer="21"/>
<wire x1="5" y1="-3" x2="-5" y2="-3" width="0.127" layer="21"/>
<wire x1="-5" y1="-3" x2="-5" y2="3" width="0.127" layer="21"/>
<wire x1="-5.25" y1="3.25" x2="5.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="5.25" y1="3.25" x2="5.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="5.25" y1="-3.25" x2="-5.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-5.25" y1="-3.25" x2="-5.25" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_10X13X10X5">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="2.5" x2="6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="2.5" x2="6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-2.5" x2="-6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-2.5" x2="-6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="2.75" x2="6.75" y2="2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="2.75" x2="6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-2.75" x2="-6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-2.75" x2="-6.75" y2="2.75" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_10X13X11X5">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="2.5" x2="6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="2.5" x2="6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-2.5" x2="-6.5" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-2.5" x2="-6.5" y2="2.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="2.75" x2="6.75" y2="2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="2.75" x2="6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-2.75" x2="-6.75" y2="-2.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-2.75" x2="-6.75" y2="2.75" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_10X13X9.5X4.5">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="2.25" x2="6.5" y2="2.25" width="0.127" layer="21"/>
<wire x1="6.5" y1="2.25" x2="6.5" y2="-2.25" width="0.127" layer="21"/>
<wire x1="6.5" y1="-2.25" x2="-6.5" y2="-2.25" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-2.25" x2="-6.5" y2="2.25" width="0.127" layer="21"/>
<wire x1="-6.75" y1="2.5" x2="6.75" y2="2.5" width="0.127" layer="39"/>
<wire x1="6.75" y1="2.5" x2="6.75" y2="-2.5" width="0.127" layer="39"/>
<wire x1="6.75" y1="-2.5" x2="-6.75" y2="-2.5" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-2.5" x2="-6.75" y2="2.5" width="0.127" layer="39"/>
<text x="-5.08" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_10X13X13X7">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="3.5" x2="6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="3.5" x2="6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-3.5" x2="-6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-3.5" x2="-6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="3.75" x2="6.75" y2="3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="3.75" x2="6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-3.75" x2="-6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-3.75" x2="-6.75" y2="3.75" width="0.127" layer="39"/>
<text x="-5.08" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_10X13X12X7">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="3.5" x2="6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="3.5" x2="6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-3.5" x2="-6.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-3.5" x2="-6.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="3.75" x2="6.75" y2="3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="3.75" x2="6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="6.75" y1="-3.75" x2="-6.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-3.75" x2="-6.75" y2="3.75" width="0.127" layer="39"/>
<text x="-5.08" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_10X13X14X8">
<pad name="1" x="-5" y="0" drill="0.9"/>
<pad name="2" x="5" y="0" drill="0.9"/>
<wire x1="-6.5" y1="4" x2="6.5" y2="4" width="0.127" layer="21"/>
<wire x1="6.5" y1="4" x2="6.5" y2="-4" width="0.127" layer="21"/>
<wire x1="6.5" y1="-4" x2="-6.5" y2="-4" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-4" x2="-6.5" y2="4" width="0.127" layer="21"/>
<wire x1="-6.75" y1="4.25" x2="6.75" y2="4.25" width="0.127" layer="39"/>
<wire x1="6.75" y1="4.25" x2="6.75" y2="-4.25" width="0.127" layer="39"/>
<wire x1="6.75" y1="-4.25" x2="-6.75" y2="-4.25" width="0.127" layer="39"/>
<wire x1="-6.75" y1="-4.25" x2="-6.75" y2="4.25" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_12.5X15X11.5X6">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="3" x2="7.5" y2="3" width="0.127" layer="21"/>
<wire x1="7.5" y1="3" x2="7.5" y2="-3" width="0.127" layer="21"/>
<wire x1="7.5" y1="-3" x2="-7.5" y2="-3" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-3" x2="-7.5" y2="3" width="0.127" layer="21"/>
<wire x1="-7.75" y1="3.25" x2="7.75" y2="3.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="3.25" x2="7.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="-3.25" x2="-7.75" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-3.25" x2="-7.75" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_12.5X15X12.5X7">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="3.5" x2="7.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="7.5" y1="3.5" x2="7.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="7.5" y1="-3.5" x2="-7.5" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-3.5" x2="-7.5" y2="3.5" width="0.127" layer="21"/>
<wire x1="-7.75" y1="3.75" x2="7.75" y2="3.75" width="0.127" layer="39"/>
<wire x1="7.75" y1="3.75" x2="7.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="7.75" y1="-3.75" x2="-7.75" y2="-3.75" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-3.75" x2="-7.75" y2="3.75" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_12.5X15X14X8.5">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="4.25" x2="7.5" y2="4.25" width="0.127" layer="21"/>
<wire x1="7.5" y1="4.25" x2="7.5" y2="-4.25" width="0.127" layer="21"/>
<wire x1="7.5" y1="-4.25" x2="-7.5" y2="-4.25" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-4.25" x2="-7.5" y2="4.25" width="0.127" layer="21"/>
<wire x1="-7.75" y1="4.5" x2="7.75" y2="4.5" width="0.127" layer="39"/>
<wire x1="7.75" y1="4.5" x2="7.75" y2="-4.5" width="0.127" layer="39"/>
<wire x1="7.75" y1="-4.5" x2="-7.75" y2="-4.5" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-4.5" x2="-7.75" y2="4.5" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_12.5X15X16X10">
<pad name="1" x="-6.25" y="0" drill="0.9"/>
<pad name="2" x="6.25" y="0" drill="0.9"/>
<wire x1="-7.5" y1="5" x2="7.5" y2="5" width="0.127" layer="21"/>
<wire x1="7.5" y1="5" x2="7.5" y2="-5" width="0.127" layer="21"/>
<wire x1="7.5" y1="-5" x2="-7.5" y2="-5" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-5" x2="-7.5" y2="5" width="0.127" layer="21"/>
<wire x1="-7.75" y1="5.25" x2="7.75" y2="5.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="5.25" x2="7.75" y2="-5.25" width="0.127" layer="39"/>
<wire x1="7.75" y1="-5.25" x2="-7.75" y2="-5.25" width="0.127" layer="39"/>
<wire x1="-7.75" y1="-5.25" x2="-7.75" y2="5.25" width="0.127" layer="39"/>
<text x="-5.08" y="6.5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-7.77" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X11X5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="2.5" x2="9" y2="2.5" width="0.127" layer="21"/>
<wire x1="9" y1="2.5" x2="9" y2="-2.5" width="0.127" layer="21"/>
<wire x1="9" y1="-2.5" x2="-9" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-9" y1="-2.5" x2="-9" y2="2.5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="2.75" x2="9.25" y2="2.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="2.75" x2="9.25" y2="-2.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="-2.75" x2="-9.25" y2="-2.75" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-2.75" x2="-9.25" y2="2.75" width="0.127" layer="39"/>
<text x="-5.08" y="4" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X12X6">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3" x2="9" y2="3" width="0.127" layer="21"/>
<wire x1="9" y1="3" x2="9" y2="-3" width="0.127" layer="21"/>
<wire x1="9" y1="-3" x2="-9" y2="-3" width="0.127" layer="21"/>
<wire x1="-9" y1="-3" x2="-9" y2="3" width="0.127" layer="21"/>
<wire x1="-9.25" y1="3.25" x2="9.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="3.25" x2="9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-3.25" x2="-9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-3.25" x2="-9.25" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="4.5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5.77" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X13.5X7.5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3.75" x2="9" y2="3.75" width="0.127" layer="21"/>
<wire x1="9" y1="3.75" x2="9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="9" y1="-3.75" x2="-9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-9" y1="-3.75" x2="-9" y2="3.75" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4" x2="9.25" y2="4" width="0.127" layer="39"/>
<wire x1="9.25" y1="4" x2="9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4" x2="-9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4" x2="-9.25" y2="4" width="0.127" layer="39"/>
<text x="-5.08" y="5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X11.5X6">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3" x2="9" y2="3" width="0.127" layer="21"/>
<wire x1="9" y1="3" x2="9" y2="-3" width="0.127" layer="21"/>
<wire x1="9" y1="-3" x2="-9" y2="-3" width="0.127" layer="21"/>
<wire x1="-9" y1="-3" x2="-9" y2="3" width="0.127" layer="21"/>
<wire x1="-9.25" y1="3.25" x2="9.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="3.25" x2="9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-3.25" x2="-9.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-3.25" x2="-9.25" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X14.5X7.5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="3.75" x2="9" y2="3.75" width="0.127" layer="21"/>
<wire x1="9" y1="3.75" x2="9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="9" y1="-3.75" x2="-9" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-9" y1="-3.75" x2="-9" y2="3.75" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4" x2="9.25" y2="4" width="0.127" layer="39"/>
<wire x1="9.25" y1="4" x2="9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4" x2="-9.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4" x2="-9.25" y2="4" width="0.127" layer="39"/>
<text x="-5.08" y="5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X14.5X8.5">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="4.25" x2="9" y2="4.25" width="0.127" layer="21"/>
<wire x1="9" y1="4.25" x2="9" y2="-4.25" width="0.127" layer="21"/>
<wire x1="9" y1="-4.25" x2="-9" y2="-4.25" width="0.127" layer="21"/>
<wire x1="-9" y1="-4.25" x2="-9" y2="4.25" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4.5" x2="9.25" y2="4.5" width="0.127" layer="39"/>
<wire x1="9.25" y1="4.5" x2="9.25" y2="-4.5" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4.5" x2="-9.25" y2="-4.5" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4.5" x2="-9.25" y2="4.5" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X14X8">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="4" x2="9" y2="4" width="0.127" layer="21"/>
<wire x1="9" y1="4" x2="9" y2="-4" width="0.127" layer="21"/>
<wire x1="9" y1="-4" x2="-9" y2="-4" width="0.127" layer="21"/>
<wire x1="-9" y1="-4" x2="-9" y2="4" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4.25" x2="9.25" y2="4.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="4.25" x2="9.25" y2="-4.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4.25" x2="-9.25" y2="-4.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4.25" x2="-9.25" y2="4.25" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X15X9">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="4.5" x2="9" y2="4.5" width="0.127" layer="21"/>
<wire x1="9" y1="4.5" x2="9" y2="-4.5" width="0.127" layer="21"/>
<wire x1="9" y1="-4.5" x2="-9" y2="-4.5" width="0.127" layer="21"/>
<wire x1="-9" y1="-4.5" x2="-9" y2="4.5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="4.75" x2="9.25" y2="4.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="4.75" x2="9.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="9.25" y1="-4.75" x2="-9.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-4.75" x2="-9.25" y2="4.75" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-7.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_15X18X16X10">
<pad name="1" x="-7.5" y="0" drill="1.1"/>
<pad name="2" x="7.5" y="0" drill="1.1"/>
<wire x1="-9" y1="5" x2="9" y2="5" width="0.127" layer="21"/>
<wire x1="9" y1="5" x2="9" y2="-5" width="0.127" layer="21"/>
<wire x1="9" y1="-5" x2="-9" y2="-5" width="0.127" layer="21"/>
<wire x1="-9" y1="-5" x2="-9" y2="5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="5.25" x2="9.25" y2="5.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="5.25" x2="9.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="9.25" y1="-5.25" x2="-9.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="-9.25" y1="-5.25" x2="-9.25" y2="5.25" width="0.127" layer="39"/>
<text x="-5.08" y="7" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X15X6">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="3" x2="13" y2="3" width="0.127" layer="21"/>
<wire x1="13" y1="3" x2="13" y2="-3" width="0.127" layer="21"/>
<wire x1="13" y1="-3" x2="-13" y2="-3" width="0.127" layer="21"/>
<wire x1="-13" y1="-3" x2="-13" y2="3" width="0.127" layer="21"/>
<wire x1="-13.25" y1="3.25" x2="13.25" y2="3.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="3.25" x2="13.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="-3.25" x2="-13.25" y2="-3.25" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-3.25" x2="-13.25" y2="3.25" width="0.127" layer="39"/>
<text x="-5.08" y="5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-5" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X16.5X7.5">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="3.75" x2="13" y2="3.75" width="0.127" layer="21"/>
<wire x1="13" y1="3.75" x2="13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="13" y1="-3.75" x2="-13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-13" y1="-3.75" x2="-13" y2="3.75" width="0.127" layer="21"/>
<wire x1="-13.25" y1="4" x2="13.25" y2="4" width="0.127" layer="39"/>
<wire x1="13.25" y1="4" x2="13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="13.25" y1="-4" x2="-13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-4" x2="-13.25" y2="4" width="0.127" layer="39"/>
<text x="-5.08" y="5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X15X7.5">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="3.75" x2="13" y2="3.75" width="0.127" layer="21"/>
<wire x1="13" y1="3.75" x2="13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="13" y1="-3.75" x2="-13" y2="-3.75" width="0.127" layer="21"/>
<wire x1="-13" y1="-3.75" x2="-13" y2="3.75" width="0.127" layer="21"/>
<wire x1="-13.25" y1="4" x2="13.25" y2="4" width="0.127" layer="39"/>
<wire x1="13.25" y1="4" x2="13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="13.25" y1="-4" x2="-13.25" y2="-4" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-4" x2="-13.25" y2="4" width="0.127" layer="39"/>
<text x="-5.08" y="5" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-6.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X18X9">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="4.5" x2="13" y2="4.5" width="0.127" layer="21"/>
<wire x1="13" y1="4.5" x2="13" y2="-4.5" width="0.127" layer="21"/>
<wire x1="13" y1="-4.5" x2="-13" y2="-4.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-4.5" x2="-13" y2="4.5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="4.75" x2="13.25" y2="4.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="4.75" x2="13.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="-4.75" x2="-13.25" y2="-4.75" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-4.75" x2="-13.25" y2="4.75" width="0.127" layer="39"/>
<text x="-5.08" y="6" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-7.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X20X11">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="5.5" x2="13" y2="5.5" width="0.127" layer="21"/>
<wire x1="13" y1="5.5" x2="13" y2="-5.5" width="0.127" layer="21"/>
<wire x1="13" y1="-5.5" x2="-13" y2="-5.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-5.5" x2="-13" y2="5.5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="5.75" x2="13.25" y2="5.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="5.75" x2="13.25" y2="-5.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="-5.75" x2="-13.25" y2="-5.75" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-5.75" x2="-13.25" y2="5.75" width="0.127" layer="39"/>
<text x="-5.08" y="7" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-8.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X21X10">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="5" x2="13" y2="5" width="0.127" layer="21"/>
<wire x1="13" y1="5" x2="13" y2="-5" width="0.127" layer="21"/>
<wire x1="13" y1="-5" x2="-13" y2="-5" width="0.127" layer="21"/>
<wire x1="-13" y1="-5" x2="-13" y2="5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="5.25" x2="13.25" y2="5.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="5.25" x2="13.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="13.25" y1="-5.25" x2="-13.25" y2="-5.25" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-5.25" x2="-13.25" y2="5.25" width="0.127" layer="39"/>
<text x="-5.08" y="7" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_22.5X26X25X15">
<pad name="1" x="-11.25" y="0" drill="1.1"/>
<pad name="2" x="11.25" y="0" drill="1.1"/>
<wire x1="-13" y1="7.5" x2="13" y2="7.5" width="0.127" layer="21"/>
<wire x1="13" y1="7.5" x2="13" y2="-7.5" width="0.127" layer="21"/>
<wire x1="13" y1="-7.5" x2="-13" y2="-7.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-7.5" x2="-13" y2="7.5" width="0.127" layer="21"/>
<wire x1="-13.25" y1="7.75" x2="13.25" y2="7.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="7.75" x2="13.25" y2="-7.75" width="0.127" layer="39"/>
<wire x1="13.25" y1="-7.75" x2="-13.25" y2="-7.75" width="0.127" layer="39"/>
<wire x1="-13.25" y1="-7.75" x2="-13.25" y2="7.75" width="0.127" layer="39"/>
<text x="-5.08" y="9" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-9" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_27.5X31X20X10.5">
<pad name="1" x="-13.75" y="0" drill="1.1"/>
<pad name="2" x="13.75" y="0" drill="1.1"/>
<wire x1="-15.5" y1="5.25" x2="15.5" y2="5.25" width="0.127" layer="21"/>
<wire x1="15.5" y1="5.25" x2="15.5" y2="-5.25" width="0.127" layer="21"/>
<wire x1="15.5" y1="-5.25" x2="-15.5" y2="-5.25" width="0.127" layer="21"/>
<wire x1="-15.5" y1="-5.25" x2="-15.5" y2="5.25" width="0.127" layer="21"/>
<wire x1="-15.75" y1="5.5" x2="15.75" y2="5.5" width="0.127" layer="39"/>
<wire x1="15.75" y1="5.5" x2="15.75" y2="-5.5" width="0.127" layer="39"/>
<wire x1="15.75" y1="-5.5" x2="-15.75" y2="-5.5" width="0.127" layer="39"/>
<wire x1="-15.75" y1="-5.5" x2="-15.75" y2="5.5" width="0.127" layer="39"/>
<text x="-5.08" y="7" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-7" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_27.5X31X22X13">
<pad name="1" x="-13.75" y="0" drill="1.1"/>
<pad name="2" x="13.75" y="0" drill="1.1"/>
<wire x1="-15.5" y1="6.5" x2="15.5" y2="6.5" width="0.127" layer="21"/>
<wire x1="15.5" y1="6.5" x2="15.5" y2="-6.5" width="0.127" layer="21"/>
<wire x1="15.5" y1="-6.5" x2="-15.5" y2="-6.5" width="0.127" layer="21"/>
<wire x1="-15.5" y1="-6.5" x2="-15.5" y2="6.5" width="0.127" layer="21"/>
<wire x1="-15.75" y1="6.75" x2="15.75" y2="6.75" width="0.127" layer="39"/>
<wire x1="15.75" y1="6.75" x2="15.75" y2="-6.75" width="0.127" layer="39"/>
<wire x1="15.75" y1="-6.75" x2="-15.75" y2="-6.75" width="0.127" layer="39"/>
<wire x1="-15.75" y1="-6.75" x2="-15.75" y2="6.75" width="0.127" layer="39"/>
<text x="-5.08" y="8" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-9.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_27.5X31X29X15.5">
<pad name="1" x="-13.75" y="0" drill="1.1"/>
<pad name="2" x="13.75" y="0" drill="1.1"/>
<wire x1="-15.5" y1="7.75" x2="15.5" y2="7.75" width="0.127" layer="21"/>
<wire x1="15.5" y1="7.75" x2="15.5" y2="-7.75" width="0.127" layer="21"/>
<wire x1="15.5" y1="-7.75" x2="-15.5" y2="-7.75" width="0.127" layer="21"/>
<wire x1="-15.5" y1="-7.75" x2="-15.5" y2="7.75" width="0.127" layer="21"/>
<wire x1="-15.75" y1="8" x2="15.75" y2="8" width="0.127" layer="39"/>
<wire x1="15.75" y1="8" x2="15.75" y2="-8" width="0.127" layer="39"/>
<wire x1="15.75" y1="-8" x2="-15.75" y2="-8" width="0.127" layer="39"/>
<wire x1="-15.75" y1="-8" x2="-15.75" y2="8" width="0.127" layer="39"/>
<text x="-5.08" y="10" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-10" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="WCAP-FTXX_37.5X41.5X35.5X22.5">
<pad name="1" x="-18.75" y="0" drill="1.3"/>
<pad name="2" x="18.75" y="0" drill="1.3"/>
<wire x1="-20.75" y1="11.25" x2="20.75" y2="11.25" width="0.127" layer="21"/>
<wire x1="20.75" y1="11.25" x2="20.75" y2="-11.25" width="0.127" layer="21"/>
<wire x1="20.75" y1="-11.25" x2="-20.75" y2="-11.25" width="0.127" layer="21"/>
<wire x1="-20.75" y1="-11.25" x2="-20.75" y2="11.25" width="0.127" layer="21"/>
<wire x1="-21" y1="11.5" x2="21" y2="11.5" width="0.127" layer="39"/>
<wire x1="21" y1="11.5" x2="21" y2="-11.5" width="0.127" layer="39"/>
<wire x1="21" y1="-11.5" x2="-21" y2="-11.5" width="0.127" layer="39"/>
<wire x1="-21" y1="-11.5" x2="-21" y2="11.5" width="0.127" layer="39"/>
<text x="-5.08" y="13" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-13" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<symbols>
<symbol name="C_POLARIZED">
<pin name="1" x="0" y="5.08" visible="pad" length="short" rot="R270"/>
<pin name="2" x="0" y="-2.54" visible="pad" length="short" rot="R90"/>
<text x="3.175" y="5.08" size="1.778" layer="95">&gt;NAME</text>
<text x="3.175" y="-3.175" size="1.778" layer="96">&gt;VALUE</text>
<wire x1="-2.54" y1="2.54" x2="2.54" y2="2.54" width="0.127" layer="94"/>
<wire x1="-2.54" y1="2.54" x2="-2.54" y2="1.905" width="0.127" layer="94"/>
<wire x1="-2.54" y1="1.905" x2="2.54" y2="1.905" width="0.127" layer="94"/>
<wire x1="2.54" y1="1.905" x2="2.54" y2="2.54" width="0.127" layer="94"/>
<wire x1="-1.905" y1="3.175" x2="-1.905" y2="4.445" width="0.127" layer="94"/>
<wire x1="-2.54" y1="3.81" x2="-1.27" y2="3.81" width="0.127" layer="94"/>
<rectangle x1="-0.3175" y1="-2.2225" x2="0.3175" y2="2.8575" layer="94" rot="R90"/>
<wire x1="-2.54" y1="-1.27" x2="-1.27" y2="-1.27" width="0.127" layer="94"/>
</symbol>
<symbol name="C_NON-POLARIZED">
<text x="2.794" y="4.191" size="1.778" layer="95">&gt;NAME</text>
<text x="2.794" y="-3.429" size="1.778" layer="96">&gt;VALUE</text>
<pin name="1" x="0" y="-2.54" visible="pad" length="short" direction="pas" rot="R90"/>
<pin name="2" x="0" y="5.08" visible="pad" length="short" direction="pas" rot="R270"/>
<rectangle x1="-1.905" y1="1.905" x2="1.905" y2="2.54" layer="94"/>
<rectangle x1="-1.905" y1="0" x2="1.905" y2="0.635" layer="94"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AS5H" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AS5H Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -40 °C to +105 °C
&lt;br&gt;Long life product series
&lt;br&gt;Load life:5000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AS5H_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AS5H_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AS5H?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AS5H?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_4X5.5(DXL)" package="2.6X1.6X1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X5.5(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X5.5(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X10.5(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X10.5(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X7.7(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ASLI Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C to +105 °C
&lt;br&gt;Low impedance product series
&lt;br&gt;Load life:2000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ASLI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ASLI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ASLI?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-ASLI?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_4X5.5(DXL)" package="2.6X1.6X1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X5.5(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X5.5(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X6.5(DXL)" package="4.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X10.5(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X10.5(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_12.5X14(DXL)" package="5.8X2.5X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X17(DXL)" package="6.5X3.5X6(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X7.7(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ASLL Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C to +105 °C
&lt;br&gt;Low impedance product series
&lt;br&gt;Load life: 2000 - 5000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ASLL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ASLL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ASLL?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-ASLL?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_4X5.5(DXL)" package="2.6X1.6X1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X5.5(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X5.5(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X10.5(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X10.5(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_12.5X14(DXL)" package="5.8X2.5X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X17(DXL)" package="6.5X3.5X6(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X7.7(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -40 °C to +85 °C
&lt;br&gt;low leakage current product series
&lt;br&gt;Load life:1000 h @ +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ASLU_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ASLU_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ASLU?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-ASLU?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_4X5.5(DXL)" package="2.6X1.6X1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X5.5(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X5.5(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X6.5(DXL)" package="4.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X7.7(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ASNP Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -40 °C to +85 °C
&lt;br&gt;Non-polarized product series with +85 °C max temperature
&lt;br&gt;Load life:2000 h @ +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ASNP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ASNP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ASNP?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-ASNP?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_NON-POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_4X5.5(DXL)" package="2.6X1.6X1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X5.5(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X5.5(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X6.5(DXL)" package="4.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X10.5(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X10.5(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X7.7(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Polymer Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C to +105 °C
&lt;br&gt;Miniaturized product series
&lt;br&gt;Low ESR at high frequency range
&lt;br&gt;High permissible ripple current
&lt;br&gt;Load life:2000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PSHP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PSHP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PSHP?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-PSHP?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_8X7.7(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X8.7(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X10.5(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X8.7(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLC" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PSLC Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Alumnium Polymer Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C to +105 °C
&lt;br&gt;Large capacitance SMD product series
&lt;br&gt;Very low ESR at high frequency range
&lt;br&gt;High permissible ripple current
&lt;br&gt;Long life and high reliability
&lt;br&gt;Load life:2000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PSLC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PSLC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PSLC?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-PSLC?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_8X11.7(DXL)" package="4.2X1.9X2.8(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.4(DXL)" package="4.4X1.9X4.3(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLP" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PSLP Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Polymer Capacitor
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C to +105 °C
&lt;br&gt;Low profile SMD product series
&lt;br&gt;Low ESR at high frequency range
&lt;br&gt;High permissible ripple current
&lt;br&gt;Load life:2000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt;Package: B X C X A = length of the solder pad X width of the solder pad X pitch of the solder pad.
&lt;br&gt;Variant: D X L = Diameter of the body part X Height of the body part. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PSLP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PSLP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PSLP?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-PSLP?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X5.5(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X5.8(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_4X5.5(DXL)" package="2.6X1.6X1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X5.8(DXL)" package="3X1.6X1.4(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X7.7(DXL)" package="3.5X1.6X2.1(BXCXA)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H" prefix="C" uservalue="yes">
<description>&lt;b&gt; WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Aluminum Electrolytic Capacitor
&lt;br&gt; Recommended soldering: Wave
&lt;br&gt; Operating temperature: -25 °C to +105 °C
&lt;br&gt; Extended lifetime product series
&lt;br&gt; Load life:3000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt; D X P X Φ = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt; Variant:
&lt;br&gt; D X L X P X Φ = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AI3H_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AI3H_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AI3H?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AI3H?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_22X26X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X36X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X46X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X51X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X26X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X31X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X36X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X41X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X46X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X26X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X31X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X36X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X41X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X51X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X32X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X37X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X42X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X52X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X57X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -25 °C to +85 °C
&lt;br&gt;Extended lifetime product series
&lt;br&gt;Load life:3000 h @ +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt; D X P X Φ = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt; Variant:
&lt;br&gt; D X L X P X Φ = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AIL8_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AIL8_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AIL8?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AIL8?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_22X26X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X36X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X46X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X26X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X31X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X36X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X41X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X26X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X31X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X36X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X41X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X46X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X27X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X32X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X37X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X42X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X47X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X52X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -25 °C to +105 °C
&lt;br&gt;General purpose product series
&lt;br&gt;High permissible ripple current
&lt;br&gt;Load life:2000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt; D X P X Φ = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt; Variant:
&lt;br&gt; D X L X P X Φ = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AIG5_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AIG5_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AIG5?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AIG5?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_22X26X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X36X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X46X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X51X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X26X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X31X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X36X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X41X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X46X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X26X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X31X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X41X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X36X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X51X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X27X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X32X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X37X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X42X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X47X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X52X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -25 °C to +85 °C
&lt;br&gt;General purpose product series
&lt;br&gt;Load life:2000 h @ +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt; D X P X Φ = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt; Variant:
&lt;br&gt; D X L X P X Φ = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AIG8_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AIG8_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AIG8?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AIG8?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_22X26X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X36X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X51X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X26X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X31X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X36X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X41X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X46X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X51X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X31X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X36X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X41X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X46X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X37X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X42X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X47X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X37X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X42X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X52X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIL5" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AIL5 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -25 °C to +105 °C
&lt;br&gt;Miniaturized product series
&lt;br&gt;High permissible ripple current
&lt;br&gt;Load life:2000 h @ +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt; D X P X Φ = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt; Variant:
&lt;br&gt; D X L X P X Φ = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AIL5_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AIL5_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AIL5?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AIL5?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_22X21X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X26X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X36X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X46X10X1.6(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X21X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X26X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X31X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X41X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X46X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X21X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X26X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X31X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X36X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X41X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X51X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X27X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X32X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X37X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X42X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X47X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X52X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X63X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X70X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIL8" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AIL8 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -25 °C to +85 °C
&lt;br&gt;Miniaturized product series
&lt;br&gt;Load life:2000 h @ +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt; Package:
&lt;br&gt; D X P X Φ = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt; Variant:
&lt;br&gt; D X L X P X Φ = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-AIL8_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-AIL8_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AIL8?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-AIL8?m
&lt;/a&gt;&lt;p&gt;Created: 2015-03-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_22X21X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X26X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X36X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X51X10X1.5(DXLXPXΦ)" package="22X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X21X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X26X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X31X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X36X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X41X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X46X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_25X56X10X1.5(DXLXPXΦ)" package="25X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X21X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X26X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X31X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X36X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_30X41X10X1.5(DXLXPXΦ)" package="30X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X27X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X32X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X37X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X42X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X47X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X57X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_35X63X10X1.5(DXLXPXΦ)" package="35X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X32X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X37X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X42X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X47X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_40X57X10X1.5(DXLXPXΦ)" package="40X10X2(DXPXΦ)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-AT1H Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -40 °C to +105 °C for UR ˂ 400 V; -25 °C to +105 °C for UR ≥ 400V
&lt;br&gt;Long life product series
&lt;br&gt;Higher permissible ripple current
&lt;br&gt;Load life: 5000-10000 h @ + 105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATIH_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATIH_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AT1H/"&gt;http://katalog.we-online.de/en/pbs/WCAP-AT1H/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X11X2X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X16X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X20X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X31.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X21X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X21X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X25X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ATET Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -40 °C to +125 °C for UR ˂ 250 V; -25 °C to +125 °C for UR ≥ 250V
&lt;br&gt;High temperature product series
&lt;br&gt;Load life: 1000-2000 h @ + 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATIH_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATIH_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AT1H/"&gt;http://katalog.we-online.de/en/pbs/WCAP-AT1H/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X25X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5X11X5X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ATG5 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -40 °C to +105 °C for UR ˂ 400 V; -25 °C to +105 °C for UR ≥ 400V
&lt;br&gt;General purpose product series with max. temperature of +105 °C
&lt;br&gt;Load life: 2000 h @ + 105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATG5_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATG5_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ATG5/"&gt;http://katalog.we-online.de/en/pbs/WCAP-ATG5/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-09
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X11X2X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X16X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X20X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X35.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X35.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X15X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X14X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X14X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X25X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X25X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X31.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X31X10X0.8(DXLXPXØ)" package="22X10X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X45X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X20X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ATG8 Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -40 °C to +85 °C for UR ˂ 400 V; -25 °C to +85 °C for UR ≥ 400V
&lt;br&gt;Wide capacitance value range
&lt;br&gt;Load life: 2000 h @ + 85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATG8_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATG8_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ATG8"&gt;http://katalog.we-online.de/en/pbs/WCAP-ATG8
&lt;/a&gt;&lt;p&gt;Created: 2015-02-06
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X11X2X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X16X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X20X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X35.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X35.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X41X10X0.8(DXLXPXØ)" package="22X10X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X31.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X41X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X25X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_22X51X10X0.8(DXLXPXØ)" package="22X10X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ATLI Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -55 °C to +105 °C 
&lt;br&gt;Low impedance product series
&lt;br&gt;Load life: 2000-5000 h @ + 105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATLI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATLI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ATLI/"&gt;http://katalog.we-online.de/en/pbs/WCAP-ATLI/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X11X2X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X16X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X20X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X20X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X25X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X15X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X30X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X35X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X35.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X31.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X30X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X21X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Electrolytic Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -55 °C to +105 °C
&lt;br&gt;Low impedance and high temperature product series
&lt;br&gt;Load life: 3000-10000 h @ + 105 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATIH_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATIH_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-AT1H/"&gt;http://katalog.we-online.de/en/pbs/WCAP-AT1H/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X11X2X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X15X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X16X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X20X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X20X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X25X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X30X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X30X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X35X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X25X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X31.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X35.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X35.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt; Aluminum Electrolytic Capacitors
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -40°C to +105°C
&lt;br&gt;Minimized ESR and long life product series  
&lt;br&gt;Load life: 4000 - 10000h @ +105°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-ATUL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-ATUL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-ATUL/"&gt;http://katalog.we-online.de/en/pbs/WCAP-ATUL/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-10
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_5X11X2X0.5(DXLXPXØ)" package="5X2X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.5(DXLXPXØ)" package="6.3X2.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X16X3.5X0.5(DXLXPXØ)" package="8X3.5X0.8(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X20X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X20X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X16X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X25X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X20X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X25X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X30X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X35X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X25X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X16X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X30X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X25X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X31.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X21X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X35.5X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X31.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_13X40X5X0.6(DXLXPXØ)" package="13X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_16X41X7.5X0.8(DXLXPXØ)" package="16X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X35.5X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_18X41X7.5X0.8(DXLXPXØ)" package="18X7.5X1.1(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PT5H" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum polymer Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -55°C to +105°C
&lt;br&gt;Long life product series with 5000 h 
&lt;br&gt;Low ESR at high frequency range
&lt;br&gt;Load life: 5000h @ +105°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PT5H_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PT5H_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PT5H/"&gt;http://katalog.we-online.de/en/pbs/WCAP-PT5H/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-06
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_8X8X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.6(DXLXPXØ)" package="6.3X2.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTG5" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PTG5 Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Polymer Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -55°C to +105°C
&lt;br&gt;Low ESR at high frequency range
&lt;br&gt;High permissible ripple current 
&lt;br&gt;Load life: 2000h @ +105°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PTG5_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PTG5_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PTG5/"&gt;http://katalog.we-online.de/en/pbs/WCAP-PTG5/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-06
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_8X8X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTHR" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PTHR Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Polymer Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -55°C to +105°C
&lt;br&gt;High reliability series
&lt;br&gt;Low ESR at high frequency range
&lt;br&gt;High permissible ripple current
&lt;br&gt;Load life: 2000h @ +105°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PTHR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PTHR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PTHR/"&gt;http://katalog.we-online.de/en/pbs/WCAP-PTHR/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-06
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_6.3X8X2.5X0.6(DXLXPXØ)" package="6.3X2.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X8X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTHT" prefix="C" uservalue="yes">
<description>&lt;b&gt;WCAP-PTHT Aluminum Polymer Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;&lt;/b&gt;Aluminum Polymer Capacitor
&lt;br&gt;Recommended soldering: Wave
&lt;br&gt;Operating temperature: -55°C to +125°C
&lt;br&gt;+125°C product series
&lt;br&gt;Low ESR at high frequency range
&lt;br&gt;Long life: 2000h @ +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Package name and Variant abbreviation:
&lt;br&gt;&lt;/b&gt;Package:
&lt;br&gt; D X A X B = Diameter of the outline X Pitch of the hole X Diameter of the  hole.
&lt;br&gt;Variant:
&lt;br&gt; D X L X P X Ø = Diameter of the body part X Height of the body part X Pitch of the pin X Diameter of the pin. 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-PTHT_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-PTHT_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-PTHT/"&gt;http://katalog.we-online.de/en/pbs/WCAP-PTHT/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-06
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_8X8X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8X11.5X3.5X0.6(DXLXPXØ)" package="8X3.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_10X12.5X5X0.6(DXLXPXØ)" package="10X5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_6.3X11X2.5X0.6(DXLXPXØ)" package="6.3X2.5X0.9(DXAXB)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP" prefix="C" uservalue="yes">
<description>&lt;b&gt; WCAP-CSGP Ceramic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Multilayer Ceramic Chip Capacitor
&lt;br&gt;Recommended soldering:Reflow, for 0603 and 0805 wave soldering is also allowed
&lt;br&gt;Operating temperature:-55 °C to +125 °C;
&lt;br&gt;Ceramic characteristics: Class I - NPO ; Class II -X7R, X5R
&lt;br&gt;High performance ceramic
&lt;br&gt;High capacitance stability
&lt;br&gt;Minimal aging 
&lt;br&gt;Termination:Cu/Ni/Sn
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-CSGP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-CSGP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-CSGP/?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-CSGP/?m
&lt;/a&gt;&lt;p&gt;Created:  2015-01-28
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_NON-POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_0402" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603-REFLOW" package="WCAP-CSGP_0603_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603-WAVE" package="WCAP-CSGP_0603_WAVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805-REFLOW" package="WCAP-CSGP_0805_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805-WAVE" package="WCAP-CSGP_0805_WAVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1206" package="WCAP-CSGP_1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1210" package="WCAP-CSGP_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1812" package="WCAP-CSGP_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSSA" prefix="C" uservalue="yes">
<description>&lt;b&gt;&lt;br&gt;WCAP-CSSA Ceramic Capacitors
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Characteristics
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt; Safety Multilayer Ceramic Chip Capacitor
&lt;br&gt;Recommended soldering: Reflow 
&lt;br&gt;Operating temperature: -55 °C to +125 °C
&lt;br&gt;NPO Capacitance characteristics: ±30ppm/°C; ±0.54%/°C
&lt;br&gt;X7R capacitance characteristics: ±15%
&lt;br&gt;Rated voltage:250V AC
&lt;br&gt;TUV/UL certified high performance ceramic
&lt;br&gt; High capacitance stability 
&lt;br&gt;Termination:Ag/Ni/Sn
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-CSSA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-CSSA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-CSSA/?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-CSSA/?m
&lt;/a&gt;&lt;p&gt;Created:  2015-01-28
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_NON-POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_1808" package="WCAP-CSSA_1808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1812" package="WCAP-CSSA_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2211" package="WCAP-CSSA_2211">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX" prefix="C" uservalue="yes">
<description>&lt;b&gt; WCAP-FTXX Film Capacitors 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;MKP,Metallized Polypropylene Film
&lt;br&gt;Recommended soldering :Wave
&lt;br&gt;Operating temperature:-40 °C to +105 °C
&lt;br&gt;Climate category: 40/105/56/B
&lt;br&gt;Self-healing properties
&lt;br&gt;Certificates: cULus, CQC, VDE
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;Safety applications
&lt;br&gt;Filter
&lt;br&gt;Power supplies
&lt;br&gt;&lt;b&gt;Electrical property
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-FTXX_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-FTXX_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/pbs/datasheet/890334022007.pdf"&gt;http://katalog.we-online.de/pbs/datasheet/890334022007.pdf&lt;/a&gt;&lt;p&gt;

Created: 2014-09-15&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_NON-POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_890334022007" package="WCAP-FTXX_7.5X11X10X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334022007CS" package="WCAP-FTXX_7.5X11X10X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334022017" package="WCAP-FTXX_7.5X10X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334022017CS" package="WCAP-FTXX_7.5X10X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023002" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023003" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023003CS" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023004" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023004CS" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023006CS" package="WCAP-FTXX_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023007" package="WCAP-FTXX_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023007CS" package="WCAP-FTXX_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023008" package="WCAP-FTXX_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023008CS" package="WCAP-FTXX_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023010" package="WCAP-FTXX_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023010CS" package="WCAP-FTXX_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023011" package="WCAP-FTXX_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023011CS" package="WCAP-FTXX_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023015" package="WCAP-FTXX_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023015CS" package="WCAP-FTXX_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023017" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023017CS" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023019" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023019CS" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023021" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023021CS" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023023CS" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023024" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023024CS" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023025" package="WCAP-FTXX_10X13X12X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023025CS" package="WCAP-FTXX_10X13X12X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023028" package="WCAP-FTXX_10X13X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023028CS" package="WCAP-FTXX_10X13X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024001" package="WCAP-FTXX_12.5X15X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024001CS" package="WCAP-FTXX_12.5X15X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024002" package="WCAP-FTXX_12.5X15X12.5X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024002CS" package="WCAP-FTXX_12.5X15X12.5X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024003" package="WCAP-FTXX_12.5X15X14X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024003CS" package="WCAP-FTXX_12.5X15X14X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024005" package="WCAP-FTXX_12.5X15X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334024005CS" package="WCAP-FTXX_12.5X15X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025004" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025006" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025009" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025011" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025013" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025015" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023002CS" package="WCAP-FTXX_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023006" package="WCAP-FTXX_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334023023" package="WCAP-FTXX_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025004CS" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025006CS" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025007CS" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025009CS" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025011CS" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025007" package="WCAP-FTXX_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025015CS" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025017" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025017CS" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025020" package="WCAP-FTXX_15X18X13.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025020CS" package="WCAP-FTXX_15X18X13.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025022" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025025" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025025CS" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025022CS" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025027" package="WCAP-FTXX_15X18X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025027CS" package="WCAP-FTXX_15X18X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025031" package="WCAP-FTXX_15X18X14.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025031CS" package="WCAP-FTXX_15X18X14.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025034" package="WCAP-FTXX_15X18X14.5X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025039" package="WCAP-FTXX_15X18X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025034CS" package="WCAP-FTXX_15X18X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025039CS" package="WCAP-FTXX_15X18X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025043" package="WCAP-FTXX_15X18X15X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025043CS" package="WCAP-FTXX_15X18X15X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025045" package="WCAP-FTXX_15X18X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025045CS" package="WCAP-FTX2_15X18X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026003" package="WCAP-FTXX_22.5X26X15X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026003CS" package="WCAP-FTXX_22.5X26X15X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026018" package="WCAP-FTXX_22.5X26X16.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026018CS" package="WCAP-FTXX_22.5X26X16.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026020" package="WCAP-FTXX_22.5X26X15X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026020CS" package="WCAP-FTXX_22.5X26X15X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026024" package="WCAP-FTXX_22.5X26X18X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026024CS" package="WCAP-FTXX_22.5X26X18X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026027" package="WCAP-FTXX_22.5X26X20X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026027CS" package="WCAP-FTXX_22.5X26X20X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026030" package="WCAP-FTXX_22.5X26X21X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026030CS" package="WCAP-FTXX_22.5X26X21X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026034" package="WCAP-FTXX_22.5X26X25X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334026034CS" package="WCAP-FTXX_22.5X26X25X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334027006" package="WCAP-FTXX_27.5X31X20X10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334027006CS" package="WCAP-FTXX_27.5X31X20X10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334027012" package="WCAP-FTXX_27.5X31X22X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334027012CS" package="WCAP-FTXX_27.5X31X22X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334027025" package="WCAP-FTXX_27.5X31X29X15.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334027025CS" package="WCAP-FTXX_27.5X31X29X15.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334028008" package="WCAP-FTX2_37.5X41.5X35.5X22.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334028008CS" package="WCAP-FTXX_37.5X41.5X35.5X22.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890334025013CS" package="WCAP-FTXX_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2" prefix="C" uservalue="yes">
<description>&lt;b&gt; WCAP-FTX2 Film Capacitors
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;MKP,Metallized Polypropylene Film
&lt;br&gt;Recommended soldering :Wave
&lt;br&gt;Operating temperature:-40 °C to +105 °C
&lt;br&gt;Climate category:40/105/56/B
&lt;br&gt;Self-healing properties
&lt;br&gt;Certificates: cULus, CQC, VDE  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Safety applications
&lt;br&gt;Filter 
&lt;br&gt;Power supplies
&lt;br&gt;

&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/WCAP-FTX2_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_WCAP-FTX2_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WCAP-FTX2/890324022007CS?m"&gt;http://katalog.we-online.de/en/pbs/WCAP-FTX2/890324022007CS?m
&lt;/a&gt;&lt;p&gt;Created:  2015-01-22
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_NON-POLARIZED" x="0" y="0"/>
</gates>
<devices>
<device name="_890324022007" package="WCAP-FTX2_7.5X11X10X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324022007CS" package="WCAP-FTX2_7.5X11X10X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324022017" package="WCAP-FTX2_7.5X10X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324022017CS" package="WCAP-FTX2_7.5X10X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023002CS" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023002" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023003" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023003CS" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023004" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023004CS" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023006" package="WCAP-FTX2_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023006CS" package="WCAP-FTX2_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023007" package="WCAP-FTX2_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023007CS" package="WCAP-FTX2_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023008" package="WCAP-FTX2_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023008CS" package="WCAP-FTX2_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023010" package="WCAP-FTX2_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023010CS" package="WCAP-FTX2_10X13X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023011" package="WCAP-FTX2_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023011CS" package="WCAP-FTX2_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023015" package="WCAP-FTX2_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023015CS" package="WCAP-FTX2_10X13X9.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023017" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023017CS" package="WCAP-FTX2_10X13X10X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023019" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023019CS" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023021" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023021CS" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023023" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023023CS" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023024" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023024CS" package="WCAP-FTX2_10X13X13X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023025" package="WCAP-FTX2_10X13X12X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023025CS" package="WCAP-FTX2_10X13X12X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023028" package="WCAP-FTX2_10X13X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324023028CS" package="WCAP-FTX2_10X13X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024001" package="WCAP-FTX2_12.5X15X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024001CS" package="WCAP-FTX2_12.5X15X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024002" package="WCAP-FTX2_12.5X15X12.5X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024002CS" package="WCAP-FTX2_12.5X15X12.5X7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024003" package="WCAP-FTX2_12.5X15X14X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024003CS" package="WCAP-FTX2_12.5X15X14X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024005" package="WCAP-FTX2_12.5X15X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324024005CS" package="WCAP-FTX2_12.5X15X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025004" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025004CS" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025006" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025006CS" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025007" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025009" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025009CS" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025011" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025011CS" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025013" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025013CS" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025015" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025015CS" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025017" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025017CS" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025020" package="WCAP-FTX2_15X18X13.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025020CS" package="WCAP-FTX2_15X18X13.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025022" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025025" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025025CS" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025027" package="WCAP-FTX2_15X18X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025027CS" package="WCAP-FTX2_15X18X11.5X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025031" package="WCAP-FTX2_15X18X14.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025034" package="WCAP-FTX2_15X18X14.5X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025039" package="WCAP-FTX2_15X18X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025039CS" package="WCAP-FTX2_15X18X14X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025043" package="WCAP-FTX2_15X18X15X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025045CS" package="WCAP-FTX2_15X18X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026003" package="WCAP-FTX2_22.5X26X15X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026003CS" package="WCAP-FTX2_22.5X26X15X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026018" package="WCAP-FTX2_22.5X26X16.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026020" package="WCAP-FTX2_22.5X26X15X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026020CS" package="WCAP-FTX2_22.5X26X15X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026024" package="WCAP-FTX2_22.5X26X18X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026024CS" package="WCAP-FTX2_22.5X26X18X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026027" package="WCAP-FTX2_22.5X26X20X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026027CS" package="WCAP-FTX2_22.5X26X20X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026034" package="WCAP-FTX2_22.5X26X25X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026034CS" package="WCAP-FTX2_22.5X26X25X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324027006" package="WCAP-FTX2_27.5X31X20X10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324027006CS" package="WCAP-FTX2_27.5X31X20X10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324027025" package="WCAP-FTX2_27.5X31X29X15.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025007CS" package="WCAP-FTX2_15X18X11X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025022CS" package="WCAP-FTX2_15X18X12X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025031CS" package="WCAP-FTX2_15X18X14.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025034CS" package="WCAP-FTX2_15X18X14.5X8.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025043CS" package="WCAP-FTX2_15X18X15X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324025045" package="WCAP-FTX2_15X18X16X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026018CS" package="WCAP-FTX2_22.5X26X16.5X7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026030" package="WCAP-FTX2_22.5X26X21X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324026030CS" package="WCAP-FTX2_22.5X26X21X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324027012" package="WCAP-FTX2_27.5X31X22X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324027012CS" package="WCAP-FTX2_27.5X31X22X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324027025CS" package="WCAP-FTX2_27.5X31X29X15.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324028008" package="WCAP-FTX2_37.5X41.5X35.5X22.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_890324028008CS" package="WCAP-FTX2_37.5X41.5X35.5X22.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
