<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;h1&gt;&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi Board&lt;/a&gt;&lt;/h1&gt;
&lt;h2&gt;Changelog&lt;/h2&gt;
&lt;ul&gt;
&lt;li&gt;2014-01-25: Added RasPi Model B Rev 2&lt;/li&gt;
&lt;li&gt;2012-01-29: Initial version from Jacques&lt;/li&gt;
&lt;/ul&gt;

&lt;h2&gt;Licence&lt;/h2&gt;
This library stands under the &lt;a href="http://www.ohwr.org/projects/cernohl/wiki"&gt;CERN Open Hardware Licence&lt;/a&gt;.

&lt;h2&gt;Authors:&lt;/h2&gt;
&lt;a href="http://www.steffenvogel.de"&gt;Steffen Vogel&lt;/a&gt;&lt;br&gt;
&lt;a href="http://www.raspberrypi.org/phpBB3/memberlist.php?mode=viewprofile&amp;u=9306"&gt;Jacques Lagnel&lt;/a&gt;
&lt;h2&gt;Links&lt;/h2&gt;
&lt;a href="http://www.raspberrypi.org/wp-content/uploads/2012/12/Raspberry-Pi-Mounting-Hole-Template.png"&gt;Mounting Holes&lt;/a&gt;&lt;br&gt;
&lt;a href="http://elinux.org/RPi_Low-level_peripherals"&gt;GPIO Description&lt;/a&gt;&lt;br&gt;
&lt;a href="http://openlab.com.au/wp-content/uploads/2013/04/Raspberry_Pi_Dimensions.png"&gt;Dimensions&lt;/a&gt;</description>
<packages>
<package name="RPI-B-V2">
</package>
<package name="RPI-B-V2-SHIELD">
</package>
<package name="RPI-B-V1">
</package>
<package name="RPI-B-V1-SHIELD">
</package>
<package name="RPI-A-SHIELD">
</package>
</packages>
<symbols>
<symbol name="RPI-B-V2">
<pin name="+3V3" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="GPIO2/I2C1_SDA"/>
<pin name="GPIO3/I2C1_SCL"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO4/GPCLK0"/>
<pin name="UART0_TXD/GPIO14"/>
<pin name="UART0_RXD/GPIO15"/>
<pin name="UART0_RTS/GPIO17"/>
<pin name="PWM0/GPIO18"/>
<pin name="GPIO27"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO10/SPI0_MOSI"/>
<pin name="GPIO9/SPI0_MISO"/>
<pin name="GPIO25"/>
<pin name="GPIO11/SPI0_SLCK"/>
<pin name="GPIO8/SPI0_CE0"/>
<pin name="GPIO7/SPI0_CE1"/>
<pin name="I2C0_SDA/GPIO28" direction="pwr"/>
<pin name="GPIO30" direction="pwr"/>
<pin name="I2C0_SCL/GPIO29" direction="pwr"/>
<pin name="GPIO31" direction="pwr"/>
<pin name="RESET" direction="pwr" function="dot"/>
</symbol>
<symbol name="RPI-B-V1">
<pin name="+3V3" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="GPIO0/I2C0_SDA"/>
<pin name="GPIO1/I2C0_SCL"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO4/GPCLK0"/>
<pin name="UART0_TXD/GPIO14"/>
<pin name="UART0_RXD/GPIO15"/>
<pin name="UART0_RTS/GPIO17"/>
<pin name="PWM0/PCM_CLK/GPIO18"/>
<pin name="PCM_DOUT/GPIO21"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO10/SPI0_MOSI"/>
<pin name="GPIO9/SPI0_MISO"/>
<pin name="GPIO25"/>
<pin name="GPIO11/SPI0_SLCK"/>
<pin name="GPIO8/SPI0_CE0"/>
<pin name="GPIO7/SPI0_CE1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RPI-B-V2">
<description>Second revision of the Model 2 board including the P5 and P6 headers.&lt;br&gt;
Mounting holes have been added.&lt;br&gt;
&lt;br&gt;
Choose the "SHIELD" variant for a predefined Dimension layer and drilling holes.&lt;br&gt;
&lt;br&gt;
Theres also a "SHIELD" variant for the Model A without a RJ45 connector.</description>
<gates>
<gate name="G$1" symbol="RPI-B-V2"/>
</gates>
<devices>
<device name="NO_SHIELD" package="RPI-B-V2">
<connects>
<connect gate="G$1" pin="+3V3" pad="P1_1 P1_17 P5_2"/>
<connect gate="G$1" pin="+5V" pad="P1_2 P1_4 P5_1"/>
<connect gate="G$1" pin="GND" pad="P1_6 P1_9 P1_14 P1_20 P1_25 P5_7 P5_8 P6_2"/>
<connect gate="G$1" pin="GPIO10/SPI0_MOSI" pad="P1_19"/>
<connect gate="G$1" pin="GPIO11/SPI0_SLCK" pad="P1_23"/>
<connect gate="G$1" pin="GPIO2/I2C1_SDA" pad="P1_3"/>
<connect gate="G$1" pin="GPIO22" pad="P1_15"/>
<connect gate="G$1" pin="GPIO23" pad="P1_16"/>
<connect gate="G$1" pin="GPIO24" pad="P1_18"/>
<connect gate="G$1" pin="GPIO25" pad="P1_22"/>
<connect gate="G$1" pin="GPIO27" pad="P1_13"/>
<connect gate="G$1" pin="GPIO3/I2C1_SCL" pad="P1_5"/>
<connect gate="G$1" pin="GPIO30" pad="P5_5"/>
<connect gate="G$1" pin="GPIO31" pad="P5_6"/>
<connect gate="G$1" pin="GPIO4/GPCLK0" pad="P1_7"/>
<connect gate="G$1" pin="GPIO7/SPI0_CE1" pad="P1_26"/>
<connect gate="G$1" pin="GPIO8/SPI0_CE0" pad="P1_24"/>
<connect gate="G$1" pin="GPIO9/SPI0_MISO" pad="P1_21"/>
<connect gate="G$1" pin="I2C0_SCL/GPIO29" pad="P5_4"/>
<connect gate="G$1" pin="I2C0_SDA/GPIO28" pad="P5_3"/>
<connect gate="G$1" pin="PWM0/GPIO18" pad="P1_12"/>
<connect gate="G$1" pin="RESET" pad="P6_1"/>
<connect gate="G$1" pin="UART0_RTS/GPIO17" pad="P1_11"/>
<connect gate="G$1" pin="UART0_RXD/GPIO15" pad="P1_10"/>
<connect gate="G$1" pin="UART0_TXD/GPIO14" pad="P1_8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHIELD" package="RPI-B-V2-SHIELD">
<connects>
<connect gate="G$1" pin="+3V3" pad="P1_1 P1_17 P5_2"/>
<connect gate="G$1" pin="+5V" pad="P1_2 P1_4 P5_1"/>
<connect gate="G$1" pin="GND" pad="P1_6 P1_9 P1_14 P1_20 P1_25 P5_7 P5_8 P6_2"/>
<connect gate="G$1" pin="GPIO10/SPI0_MOSI" pad="P1_19"/>
<connect gate="G$1" pin="GPIO11/SPI0_SLCK" pad="P1_23"/>
<connect gate="G$1" pin="GPIO2/I2C1_SDA" pad="P1_3"/>
<connect gate="G$1" pin="GPIO22" pad="P1_15"/>
<connect gate="G$1" pin="GPIO23" pad="P1_16"/>
<connect gate="G$1" pin="GPIO24" pad="P1_18"/>
<connect gate="G$1" pin="GPIO25" pad="P1_22"/>
<connect gate="G$1" pin="GPIO27" pad="P1_13"/>
<connect gate="G$1" pin="GPIO3/I2C1_SCL" pad="P1_5"/>
<connect gate="G$1" pin="GPIO30" pad="P5_5"/>
<connect gate="G$1" pin="GPIO31" pad="P5_6"/>
<connect gate="G$1" pin="GPIO4/GPCLK0" pad="P1_7"/>
<connect gate="G$1" pin="GPIO7/SPI0_CE1" pad="P1_26"/>
<connect gate="G$1" pin="GPIO8/SPI0_CE0" pad="P1_24"/>
<connect gate="G$1" pin="GPIO9/SPI0_MISO" pad="P1_21"/>
<connect gate="G$1" pin="I2C0_SCL/GPIO29" pad="P5_4"/>
<connect gate="G$1" pin="I2C0_SDA/GPIO28" pad="P5_3"/>
<connect gate="G$1" pin="PWM0/GPIO18" pad="P1_12"/>
<connect gate="G$1" pin="RESET" pad="P6_1"/>
<connect gate="G$1" pin="UART0_RTS/GPIO17" pad="P1_11"/>
<connect gate="G$1" pin="UART0_RXD/GPIO15" pad="P1_10"/>
<connect gate="G$1" pin="UART0_TXD/GPIO14" pad="P1_8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="RPI-A-SHIELD">
<connects>
<connect gate="G$1" pin="+3V3" pad="P1_1 P1_17 P5_2"/>
<connect gate="G$1" pin="+5V" pad="P1_2 P1_4 P5_1"/>
<connect gate="G$1" pin="GND" pad="P1_6 P1_9 P1_14 P1_20 P1_25 P5_7 P5_8 P6_2"/>
<connect gate="G$1" pin="GPIO10/SPI0_MOSI" pad="P1_19"/>
<connect gate="G$1" pin="GPIO11/SPI0_SLCK" pad="P1_23"/>
<connect gate="G$1" pin="GPIO2/I2C1_SDA" pad="P1_3"/>
<connect gate="G$1" pin="GPIO22" pad="P1_15"/>
<connect gate="G$1" pin="GPIO23" pad="P1_16"/>
<connect gate="G$1" pin="GPIO24" pad="P1_18"/>
<connect gate="G$1" pin="GPIO25" pad="P1_22"/>
<connect gate="G$1" pin="GPIO27" pad="P1_13"/>
<connect gate="G$1" pin="GPIO3/I2C1_SCL" pad="P1_5"/>
<connect gate="G$1" pin="GPIO30" pad="P5_5"/>
<connect gate="G$1" pin="GPIO31" pad="P5_6"/>
<connect gate="G$1" pin="GPIO4/GPCLK0" pad="P1_7"/>
<connect gate="G$1" pin="GPIO7/SPI0_CE1" pad="P1_26"/>
<connect gate="G$1" pin="GPIO8/SPI0_CE0" pad="P1_24"/>
<connect gate="G$1" pin="GPIO9/SPI0_MISO" pad="P1_21"/>
<connect gate="G$1" pin="I2C0_SCL/GPIO29" pad="P5_4"/>
<connect gate="G$1" pin="I2C0_SDA/GPIO28" pad="P5_3"/>
<connect gate="G$1" pin="PWM0/GPIO18" pad="P1_12"/>
<connect gate="G$1" pin="RESET" pad="P6_1"/>
<connect gate="G$1" pin="UART0_RTS/GPIO17" pad="P1_11"/>
<connect gate="G$1" pin="UART0_RXD/GPIO15" pad="P1_10"/>
<connect gate="G$1" pin="UART0_TXD/GPIO14" pad="P1_8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RPI-B-V1">
<description>First revision of the Model B board without P5 and P6 headers and mounting holes.&lt;br&gt;
Choose the "SHIELD" variant for a predefined Dimension layer.</description>
<gates>
<gate name="G$1" symbol="RPI-B-V1"/>
</gates>
<devices>
<device name="" package="RPI-B-V1">
<connects>
<connect gate="G$1" pin="+3V3" pad="P1_1 P1_17"/>
<connect gate="G$1" pin="+5V" pad="P1_2 P1_4"/>
<connect gate="G$1" pin="GND" pad="P1_6 P1_9 P1_14 P1_20 P1_25"/>
<connect gate="G$1" pin="GPIO0/I2C0_SDA" pad="P1_3"/>
<connect gate="G$1" pin="GPIO1/I2C0_SCL" pad="P1_5"/>
<connect gate="G$1" pin="GPIO10/SPI0_MOSI" pad="P1_19"/>
<connect gate="G$1" pin="GPIO11/SPI0_SLCK" pad="P1_23"/>
<connect gate="G$1" pin="GPIO22" pad="P1_15"/>
<connect gate="G$1" pin="GPIO23" pad="P1_16"/>
<connect gate="G$1" pin="GPIO24" pad="P1_18"/>
<connect gate="G$1" pin="GPIO25" pad="P1_22"/>
<connect gate="G$1" pin="GPIO4/GPCLK0" pad="P1_7"/>
<connect gate="G$1" pin="GPIO7/SPI0_CE1" pad="P1_26"/>
<connect gate="G$1" pin="GPIO8/SPI0_CE0" pad="P1_24"/>
<connect gate="G$1" pin="GPIO9/SPI0_MISO" pad="P1_21"/>
<connect gate="G$1" pin="PCM_DOUT/GPIO21" pad="P1_13"/>
<connect gate="G$1" pin="PWM0/PCM_CLK/GPIO18" pad="P1_12"/>
<connect gate="G$1" pin="UART0_RTS/GPIO17" pad="P1_11"/>
<connect gate="G$1" pin="UART0_RXD/GPIO15" pad="P1_10"/>
<connect gate="G$1" pin="UART0_TXD/GPIO14" pad="P1_8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHIELD" package="RPI-B-V1-SHIELD">
<connects>
<connect gate="G$1" pin="+3V3" pad="P1_1 P1_17"/>
<connect gate="G$1" pin="+5V" pad="P1_2 P1_4"/>
<connect gate="G$1" pin="GND" pad="P1_6 P1_9 P1_14 P1_20 P1_25"/>
<connect gate="G$1" pin="GPIO0/I2C0_SDA" pad="P1_3"/>
<connect gate="G$1" pin="GPIO1/I2C0_SCL" pad="P1_5"/>
<connect gate="G$1" pin="GPIO10/SPI0_MOSI" pad="P1_19"/>
<connect gate="G$1" pin="GPIO11/SPI0_SLCK" pad="P1_23"/>
<connect gate="G$1" pin="GPIO22" pad="P1_15"/>
<connect gate="G$1" pin="GPIO23" pad="P1_16"/>
<connect gate="G$1" pin="GPIO24" pad="P1_18"/>
<connect gate="G$1" pin="GPIO25" pad="P1_22"/>
<connect gate="G$1" pin="GPIO4/GPCLK0" pad="P1_7"/>
<connect gate="G$1" pin="GPIO7/SPI0_CE1" pad="P1_26"/>
<connect gate="G$1" pin="GPIO8/SPI0_CE0" pad="P1_24"/>
<connect gate="G$1" pin="GPIO9/SPI0_MISO" pad="P1_21"/>
<connect gate="G$1" pin="PCM_DOUT/GPIO21" pad="P1_13"/>
<connect gate="G$1" pin="PWM0/PCM_CLK/GPIO18" pad="P1_12"/>
<connect gate="G$1" pin="UART0_RTS/GPIO17" pad="P1_11"/>
<connect gate="G$1" pin="UART0_RXD/GPIO15" pad="P1_10"/>
<connect gate="G$1" pin="UART0_TXD/GPIO14" pad="P1_8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
