<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Elements&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015b, 08.04.2015&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="7.8MM_PAD_NO-HOLE">
<description>7.8mm Solderpad</description>
</package>
<package name="8.2MMPAD+1.2MMTHRH+10MMCU">
<description>8.2mm Solderpad, 1.2mm drill hole, 8.2-&gt;10mm Soldermask over Cu</description>
</package>
<package name="8MM_PAD_WITH_1.2MM_THRH">
<description>8mm Solderpad with 1.2mm Non Plated Through Hole</description>
</package>
<package name="8.2MMPAD+1.2MMTHRH+10MMCU+8DK">
<description>8.2mm Solderpad, 1.2mm drill hole, 8.2-&gt;10mm soldermask over Cu, 8 Vias 0.4mm</description>
</package>
<package name="8.2MM_PAD+4.2MM_THRH">
<description>8.2mm Solderpad with 4.2mm Non Plated Drill Hole</description>
</package>
<package name="8.2MM_PAD+5.2MM_THRH">
<description>8.2mm Solderpad with 5.2mm Non Plated Drill Hole</description>
</package>
<package name="8PINS_CIR">
</package>
<package name="8PINS_CIR_HAL">
</package>
<package name="12PINS_CIR">
</package>
<package name="12PINS_CIR_HAL">
</package>
<package name="16PINS_CIR">
</package>
<package name="16PINS_CIR_HAL">
</package>
<package name="20PINS_CIR">
</package>
<package name="20PINS_CIR_HAL">
</package>
<package name="36PINS_FULL">
</package>
<package name="36PINS_FULL_HAL">
</package>
<package name="4PINS_5X5_FULL">
</package>
<package name="4PINS_5X5_FULL_HAL">
</package>
<package name="9PINS_FULL">
</package>
<package name="9PINS_FULL_HAL">
</package>
<package name="16PINS_9X9_FULL">
</package>
<package name="16PINS_9X9_FULL_HAL">
</package>
<package name="16PINS_10X10_FULL">
</package>
<package name="16PINS_10X10_FULL_HAL">
</package>
<package name="25PINS_FULL">
</package>
<package name="25PINS_FULL_HAL">
</package>
<package name="6PINS_TWOROW">
</package>
<package name="6PINS_TWOROW_HAL">
</package>
<package name="8PINS_9X9_TWOROW">
</package>
<package name="8PINS_9X9_TWOROWS_HAL">
</package>
<package name="10PINS_TWOROW">
</package>
<package name="10PINS_TWOROW_HAL">
</package>
<package name="12PINS_TWOROW">
</package>
<package name="12PINS_TWOROW_HAL">
</package>
<package name="8PINS_10X10_TWOROWS_HAL">
</package>
<package name="8PINS_10X10_TWOROW">
</package>
<package name="74722715">
</package>
<package name="7470038">
</package>
<package name="7470075">
</package>
<package name="7470295">
</package>
<package name="7470466">
</package>
<package name="74722015">
</package>
<package name="74722020">
</package>
<package name="74760045">
</package>
<package name="74760050">
</package>
<package name="74722720">
</package>
<package name="10PINS_TWOROW(O)">
</package>
<package name="8PINS_TWOROW(N)">
</package>
<package name="8PINS_TWOROWS(N)_HAL">
</package>
<package name="10PIN_TWOROW(O)_HAL">
</package>
<package name="12PINS_TWOROW(P)_HAL">
</package>
<package name="12PINS_TWOROW(P)">
</package>
<package name="12PINS_TWOROW(Q)_HAL">
</package>
<package name="12PINS_TWOROW(Q)">
</package>
</packages>
<symbols>
<symbol name="WE-SMBU">
<description>BUSH</description>
<pin name="P$1"/>
</symbol>
<symbol name="WE-SMSH">
<description>SHANK</description>
<pin name="P$1"/>
</symbol>
<symbol name="PRESSFIT">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WP_SMBU" prefix="E" uservalue="yes">
<description>SMD Power Elements&lt;PRE&gt;</description>
<gates>
<gate name="G$1" symbol="WE-SMBU"/>
</gates>
<devices>
<device name="-7466003" package="8.2MM_PAD+4.2MM_THRH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466004" package="8.2MM_PAD+5.2MM_THRH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466203" package="7.8MM_PAD_NO-HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466204" package="7.8MM_PAD_NO-HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466103" package="8MM_PAD_WITH_1.2MM_THRH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466104" package="8MM_PAD_WITH_1.2MM_THRH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-SMSH" prefix="E">
<description>SMD Power Elements&lt;PRE&gt;</description>
<gates>
<gate name="G$1" symbol="WE-SMSH"/>
</gates>
<devices>
<device name="-7466213" package="7.8MM_PAD_NO-HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466214" package="7.8MM_PAD_NO-HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466113" package="8MM_PAD_WITH_1.2MM_THRH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7466114" package="8MM_PAD_WITH_1.2MM_THRH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-BUCF" prefix="E" uservalue="yes">
<description>&lt;b&gt; Bush with 
Pin-Plate Circumferences
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;MATERIAL:CuZn39Pb3
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
CIR means  Bush with Pin-Plate Circumferences&lt;br&gt;
F,G,H,E means Format Type&lt;br&gt;
HAL means Land pattern for HAL &lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-BUCF.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-BUCF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/Powerbuchsen_rundumlaufend/7461148?m"&gt;http://katalog.we-online.de/en/em/Powerbuchsen_rundumlaufend/7461148?m&lt;/a&gt;&lt;p&gt;


&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_E" package="8PINS_CIR">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E(HAL)" package="8PINS_CIR_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_F" package="12PINS_CIR">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_F(HAL)" package="12PINS_CIR_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_G" package="16PINS_CIR">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_G(HAL)" package="16PINS_CIR_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_H" package="20PINS_CIR">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_H(HAL)" package="20PINS_CIR_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-BUFU" prefix="E" uservalue="yes">
<description>&lt;b&gt; Bush with 
full plain Pin-Plate
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;MATERIAL:CuZn39Pb3
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
FULL means  Bush with full plain Pin-Plate&lt;br&gt;
J,K,L,G,I means Format Type&lt;br&gt;
10X10,9X9,5X5 means Dimensions of Procucts
J(10) means format type is J ,Dimension of product is 10mm.
J(9)means format type is J ,Dimension of product is 9mm.
HAL means Land pattern for HAL &lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-BUFU.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-BUFU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/Powerbuchsen_vollflaechig/7462810?m"&gt;http://katalog.we-online.de/en/em/Powerbuchsen_vollflaechig/7462810?m&lt;/a&gt;&lt;p&gt;


&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_L" package="36PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_L(HAL)" package="36PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_G" package="4PINS_5X5_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_G(HAL)" package="4PINS_5X5_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_I" package="9PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_I(HAL)" package="9PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J(9)" package="16PINS_9X9_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J(9)(HAL)" package="16PINS_9X9_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J(10)" package="16PINS_10X10_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J(10)(HAL)" package="16PINS_10X10_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_K" package="25PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_K(HAL)" package="25PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-BUTR" prefix="E" uservalue="yes">
<description>&lt;b&gt; Bush with 
two Rows Pin-Plate
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;MATERIAL:CuZn39Pb3
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
TWOROW means  Bush with two Rows Pin-Plate&lt;br&gt;
A,B,C,D means Format Type&lt;br&gt;
10X10,9X9 means Dimensions of Procucts
B(10) means format type is B ,Dimension of product is 10mm.
B(9)means format type is B ,Dimension of product is 9mm.
HAL means Land pattern for HAL &lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-BUTR.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-BUTR.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/Powerbuchsen_zweireihig/7461057?m"&gt;http://katalog.we-online.de/en/em/Powerbuchsen_zweireihig/7461057?m&lt;/a&gt;&lt;p&gt;

&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_A" package="6PINS_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_A(HAL)" package="6PINS_TWOROW_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_B(9)" package="8PINS_9X9_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_B(9)(HAL)" package="8PINS_9X9_TWOROWS_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_C" package="10PINS_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_C(HAL)" package="10PINS_TWOROW_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_D" package="12PINS_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_D(HAL)" package="12PINS_TWOROW_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_B(10)(HAL)" package="8PINS_10X10_TWOROWS_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_B(10)" package="8PINS_10X10_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-FLEP" prefix="E" uservalue="yes">
<description>&lt;b&gt; Power Elements with Press-Fit Technique with flexible Pin WP-FLEP
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Terminal:Naterial CuSn6
&lt;br&gt; Surface:plated with2Um Sn
&lt;br&gt;Square Nut:Material CuZn30Pb3
&lt;br&gt; Surface:2Um Nickel,Plated with 4Um SnPD
&lt;br&gt;Prepared hole diameter:1.75(+0.025/-0.025)mm
&lt;br&gt; Final hole diamerer:1.6(+0.09/-0.06)mm
&lt;br&gt;PCB 1.6mm-3.2mm
&lt;br&gt;Connection possibilities:Nut,bolt,spade orring terminal and doldered installation possibel
&lt;br&gt;
&lt;br&gt;Installation of power tracks possible
&lt;br&gt;Insertion FORCE:MIN.250n,MAX,1000n 
&lt;br&gt; Tightening force:1.3Nm
&lt;br&gt; Curent rating*:45A(20°C)
&lt;br&gt;                30A(70°C)
&lt;br&gt;                20A(100°C)
&lt;br&gt;* Operating current is defined by the PCB,heat distrbution,cable diameter and cable shoe.
&lt;br&gt;               
&lt;br&gt; 
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-FLEP.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-FLEP.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/Powerelemente_mit_flexiblen_Pins/74760045?m"&gt;http://katalog.we-online.de/en/em/Powerelemente_mit_flexiblen_Pins/74760045?m&lt;/a&gt;&lt;p&gt;

&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_74722715" package="74722715">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7470038" package="7470038">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7470075" package="7470075">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7470295" package="7470295">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7470466" package="7470466">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74722015" package="74722015">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74722020" package="74722020">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="74760045" package="74760045">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74760050" package="74760050">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74722720" package="74722720">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-RAFU" prefix="E" uservalue="yes">
<description>&lt;b&gt; Power Element 90° with 
full plain Pin-Plate
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;MATERIAL:CuZn39Pb3
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
FULL means  Power Element 90° with 
full plain Pin-Plate&lt;br&gt;
J,K,L,I means Format Type&lt;br&gt;
HAL means Land pattern for HAL &lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-RAFU_Power_Elements_90_746xxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-RAFU_Power_Elements_90_746xxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/90_abgewinkelte_Powerelemente_vollflaechig/7461066?mm"&gt;http://katalog.we-online.de/en/em/90_abgewinkelte_Powerelemente_vollflaechig/7461066?m&lt;/a&gt;&lt;p&gt;


&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_I" package="9PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_I(HAL)" package="9PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J" package="16PINS_9X9_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J(HAL)" package="16PINS_9X9_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_K" package="25PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_K(HAL)" package="25PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_L" package="36PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_L(HAL)" package="36PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-RATR" prefix="E" uservalue="yes">
<description>&lt;b&gt; Power Element 90° with two Rows Pin-Plate
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;MATERIAL:CuZn39Pb3
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
TWOROW means Power Element 90° with two Rows Pin-Plate&lt;br&gt;
A,B,C means Format Type&lt;br&gt;
HAL means Land pattern for HAL &lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-RATR.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-RATR.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/90_abgewinkelte_Powerelemente_zweireihig/7461101?m"&gt;http://katalog.we-online.de/en/em/90_abgewinkelte_Powerelemente_zweireihig/7461101?m&lt;/a&gt;&lt;p&gt;

&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_A" package="6PINS_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_A(HAL)" package="6PINS_TWOROW_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_B" package="8PINS_9X9_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_B(HAL)" package="8PINS_9X9_TWOROWS_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_C" package="10PINS_TWOROW">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_C(HAL)" package="10PINS_TWOROW_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-SHFU" prefix="E" uservalue="yes">
<description>&lt;b&gt; Threaded shank with full plain Pin-Plate
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;MATERIAL:CuZn39Pb3
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
FULL means Threaded shank with full plain Pin-Plate&lt;br&gt;
J,K,L,I means Format Type&lt;br&gt;
HAL means Land pattern for HAL &lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-SHFU.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-SHFU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/Powerelemente_mit_Gewindestift_vollflaechig/7461094?m"&gt;http://katalog.we-online.de/en/em/Powerelemente_mit_Gewindestift_vollflaechig/7461094?m&lt;/a&gt;&lt;p&gt;

&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_K" package="25PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_K(HAL)" package="25PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_I" package="9PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_I(HAL)" package="9PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J" package="16PINS_9X9_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_J(HAL)" package="16PINS_9X9_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_L" package="36PINS_FULL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_L(HAL)" package="36PINS_FULL_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-TGTR" prefix="E" uservalue="yes">
<description>&lt;b&gt; Ground Element with  two Rows Pin-Plate
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt; Drill hole diameter:1.60(-0.03)mm
&lt;br&gt; Final hole diameter 
&lt;br&gt;for HAL surface:1.45(+/-0.05)mm
&lt;br&gt; forchemical tin:1.475(+/-0.05)mm
&lt;br&gt;Min. layer thickness of copper in the via:25UM
&lt;br&gt; Max.layer thickness of tin in the via:15UM
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Advantages:
&lt;br&gt;&lt;/b&gt; High current Board-to-Board connection
&lt;br&gt; Double secured against solving
&lt;br&gt; Very low height
&lt;br&gt; Flexible connection possibilities:threaded shank,threaded hole and through hole 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
TWOROW means Ground Element with  two Rows Pin-Plate&lt;br&gt;
O,P,Q,N means Format Type&lt;br&gt;
HAL means Land pattern for HAL &lt;br&gt;

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WP-TGTR(3).jpg="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WP-TGTR(3).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/Zweiteilige_Powerelemente_Grundelement/7461070?m"&gt;http://katalog.we-online.de/en/em/Zweiteilige_Powerelemente_Grundelement/7461070?m&lt;/a&gt;&lt;p&gt;

&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_O" package="10PINS_TWOROW(O)">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_N" package="8PINS_TWOROW(N)">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_N(HAL)" package="8PINS_TWOROWS(N)_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_O(HAL)" package="10PIN_TWOROW(O)_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_P(HAL)" package="12PINS_TWOROW(P)_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_P" package="12PINS_TWOROW(P)">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_Q(HAL)" package="12PINS_TWOROW(Q)_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_Q" package="12PINS_TWOROW(Q)">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
