description[de] = <b>EAGLE Design Rules</b>\n<p>\nDie Standard-Design-Rules sind so gewählt, dass sie für \ndie meisten Anwendungen passen. Sollte ihre Platine \nbesondere Anforderungen haben, treffen Sie die erforderlichen\nEinstellungen hier und speichern die Design Rules unter \neinem neuen Namen ab.
description[en] = <b>EAGLE Design Rules</b>\n<p>\nThe default Design Rules have been set to cover\na wide range of applications. Your particular design\nmay have different requirements, so please make the\nnecessary adjustments and save your customized\ndesign rules under a new name.
description[zh] = <b>Seeed Studio EAGLE Design Rules</b>\n
layerSetup = (1*16)
mtCopper = 0.035mm 0.0175mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.0175mm 0.035mm
mtIsolate = 1.5mm 1.1mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm
mdWireWire = 6mil
mdWirePad = 6mil
mdWireVia = 6mil
mdPadPad = 6mil
mdPadVia = 6mil
mdViaVia = 6mil
mdSmdPad = 0mil
mdSmdVia = 0mil
mdSmdSmd = 0mil
mdViaViaSameLayer = 8mil
mnLayersViaInSmd = 2
mdCopperDimension = 10mil
mdDrill = 10mil
mdSmdStop = 0mil
msWidth = 6mil
msDrill = 12mil
msMicroVia = 12mil
msBlindViaRatio = 0.500000
rvPadTop = 0.250000
rvPadInner = 0.250000
rvPadBottom = 0.250000
rvViaOuter = 0.250000
rvViaInner = 0.250000
rvMicroViaOuter = 0.250000
rvMicroViaInner = 0.250000
rlMinPadTop = 10mil
rlMaxPadTop = 20mil
rlMinPadInner = 10mil
rlMaxPadInner = 20mil
rlMinPadBottom = 10mil
rlMaxPadBottom = 20mil
rlMinViaOuter = 6mil
rlMaxViaOuter = 20mil
rlMinViaInner = 6mil
rlMaxViaInner = 20mil
rlMinMicroViaOuter = 4mil
rlMaxMicroViaOuter = 20mil
rlMinMicroViaInner = 4mil
rlMaxMicroViaInner = 20mil
psTop = -1
psBottom = -1
psFirst = 0
psElongationLong = 100
psElongationOffset = 100
mvStopFrame = 1.000000
mvCreamFrame = 0.000000
mlMinStopFrame = 2mil
mlMaxStopFrame = 2mil
mlMinCreamFrame = 0mil
mlMaxCreamFrame = 0mil
mlViaStopLimit = 100mil
srRoundness = 0.000000
srMinRoundness = 0mil
srMaxRoundness = 0mil
slThermalIsolate = 10mil
slThermalsForVias = 0
dpMaxLengthDifference = 10mm
dpGapFactor = 2.500000
checkGrid = 0
checkAngle = 0
checkFont = 1
checkRestrict = 0
useDiameter = 13
maxErrors = 50
